i=1
for lines in `cat ./boot/mark`
do
  case ${i} in
  1) var1=${lines};;
  esac
  i=`expr ${i} + 1`
done
#echo "$var1"

j=$(uname -n)
if test "$var1" = "0" -a "$1" != "lite" -a "$2" != "lite" ;then

if test "$j" != "retropie" ;then
sudo apt-get install xserver-xorg-input-evdev
sudo cp -rf /usr/share/X11/xorg.conf.d/10-evdev.conf /usr/share/X11/xorg.conf.d/45-evdev.conf
fi

if test "$j" = "retropie" ;then
sudo cp -rf ./nes /home/pi/RetroPie/roms/

sudo mkdir -p /usr/src/mk_arcade_joystick_rpi-0.1.5/
sudo mkdir -p /etc/modprobe.d/
sudo cp -a ./mk_arcade_joystick_rpi-master/* /usr/src/mk_arcade_joystick_rpi-0.1.5/
export MKVERSION=0.1.5
sudo -E dkms build -m mk_arcade_joystick_rpi -v 0.1.5
sudo -E dkms install -m mk_arcade_joystick_rpi -v 0.1.5
sudo cp -rf ./etc/modules /etc/modules
sudo cp -rf ./etc/modprobe.d/joystick.conf /etc/modprobe.d/

fi

echo "1" > ./boot/mark
sudo dpkg -i -B ./xinput-calibrator_0.7.5-1_armhf.deb
sudo apt-get install cmake -y
cd ./rpi-fbcp/build/
sudo cmake ..
sudo make
sudo install fbcp /usr/local/bin/fbcp
cd ../../
sudo mkdir -p /usr/share/X11/xorg.conf.d

elif test "$var1" = "0" -a "$1" = "lite" ;then
echo "1" > ./boot/mark
echo "No touch driver installled"
echo "No fbcp driver installled"
sudo mkdir -p /usr/share/X11/xorg.conf.d

fi

if test "$j" != "kali" ;then
if test "$1" != "lite" -a "$2" != "lite" ;then
sudo cp -rf ./usr/share/X11/xorg.conf.d/99-fbturbo.conf-HDMI  /usr/share/X11/xorg.conf.d/99-fbturbo.conf
else
sudo cp -rf ./usr/share/X11/xorg.conf.d/99-fbturbo.conf  /usr/share/X11/xorg.conf.d/99-fbturbo.conf
fi
else
sudo cp ./usr/share/X11/xorg.conf.d/99-fbturbo.conf-kali /usr/share/X11/xorg.conf.d/99-fbturbo.conf
fi

sudo cp ./etc/modules /etc/


sudo cp -rf ./etc/rc.local-154 /etc/rc.local


if test "$1" = "0" -o "$#" = "0" -o "$2" = "0";then
	sudo cp -rf ./etc/X11/xorg.conf.d/99-calibration.conf-154  /usr/share/X11/xorg.conf.d/99-calibration.conf
	sudo cp ./boot/config-154.txt /boot/config.txt
	echo "LCD configrue 0"
elif test "$1" = "lite" -a "$#" = "1" ;then
        sudo cp -rf ./etc/X11/xorg.conf.d/99-calibration.conf-154  /usr/share/X11/xorg.conf.d/99-calibration.conf
        sudo cp ./boot/config-154.txt /boot/config.txt
        echo "LCD configrue 0"
elif test "$1" = "90" -o "$2" = "90";then
	if test "$1" = "lite" -o "$2" = "lite" -o "$j" = "kali" ; then
	sudo cp ./boot/config-154.txt /boot/config.txt
	sudo cp -rf ./etc/rc.local-154-90 /etc/rc.local
	else
	sudo cp ./boot/config-154.txt-90 /boot/config.txt
	fi
	sudo cp -rf ./etc/X11/xorg.conf.d/99-calibration.conf-154-90  /usr/share/X11/xorg.conf.d/99-calibration.conf
	echo "LCD configrue 90"
fi

if [ -b /dev/mmcblk0p7 ]; then
sudo cp ./cmdline.txt-noobs /boot/cmdline.txt
else
sudo cp ./cmdline.txt /boot/
fi

sudo cp ./inittab /etc/


if test "$#" = "0" -o "$1" = "0" -o "$1" = "90"  -o "$1" = "180" -o "$1" = "270" -o "$2" = "0" -o "$2" = "90"  -o "$2" = "180" -o "$2" = "270" -o "$1" = "lite" -o "$2" = "lite" ; then
sudo reboot
echo "reboot now"
else
echo "Invalid parameter,Usage:LCD154-show [0] [90] [180] [270] [lite]"
fi
