<?xml version="1.0"?>
<!DOCTYPE multimedia-project>
<multimediaproject creator="Linux MultiMedia Studio (LMMS)" creatorversion="0.2.1-svn20060925" type="song" version="1.0" >
<head>
<automation-pattern>
<bpm>
<time value="140" pos="0" />
</bpm>
<mastervol>
<time value="38" pos="0" />
</mastervol>
<masterpitch>
<time value="0" pos="0" />
</masterpitch>
</automation-pattern>
</head>
<song>
<trackcontainer width="748" x="160" y="15" height="503" type="songeditor" visible="1" >
<track muted="0" height="32" type="1" >
<bbtrack icon="" name="start of lap" >
<trackcontainer width="504" x="194" y="214" height="300" type="bbeditor" visible="1" >
<track muted="0" height="32" type="0" >
<instrumenttrack width="250" x="514" y="199" height="436" name="bassdrum02.ogg" tab="1" visible="0" >
<automation-pattern>
<vol>
<time value="200" pos="0" />
</vol>
<surpos-x>
<time value="0" pos="0" />
</surpos-x>
<surpos-y>
<time value="0" pos="0" />
</surpos-y>
<fxch>
<time value="0" pos="0" />
</fxch>
<basenote>
<time value="57" pos="0" />
</basenote>
</automation-pattern>
<audiofileprocessor reversed="0" looped="0" eframe="0.997872" sframe="0" amp="130" src="drums/bassdrum02.ogg" />
<eldata fwet="1" >
<automation-pattern>
<ftype>
<time value="7" pos="0" />
</ftype>
<fcut>
<time value="2560" pos="0" />
</fcut>
<fres>
<time value="0.69" pos="0" />
</fres>
</automation-pattern>
<elvol syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.992" pos="0" />
</hold>
<dec>
<time value="0.2" pos="0" />
</dec>
<sus>
<time value="0.679" pos="0" />
</sus>
<rel>
<time value="0.924" pos="0" />
</rel>
<amt>
<time value="1" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elvol>
<elcut syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0.392" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.938" pos="0" />
</hold>
<dec>
<time value="0.479" pos="0" />
</dec>
<sus>
<time value="0.479" pos="0" />
</sus>
<rel>
<time value="0.355" pos="0" />
</rel>
<amt>
<time value="-0.195" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elcut>
<elres syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0.035" pos="0" />
</att>
<hold>
<time value="0.892" pos="0" />
</hold>
<dec>
<time value="0.479" pos="0" />
</dec>
<sus>
<time value="0.544" pos="0" />
</sus>
<rel>
<time value="0.61" pos="0" />
</rel>
<amt>
<time value="1" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elres>
</eldata>
<arpandchords arpdisabled="1" syncmode="0" chorddisabled="1" >
<automation-pattern>
<chord>
<time value="0" pos="0" />
</chord>
<chordrange>
<time value="2" pos="0" />
</chordrange>
<arp>
<time value="0" pos="0" />
</arp>
<arprange>
<time value="1" pos="0" />
</arprange>
<arptime>
<time value="1000" pos="0" />
</arptime>
<arptime_numerator>
<time value="1" pos="0" />
</arptime_numerator>
<arptime_denominator>
<time value="1" pos="0" />
</arptime_denominator>
<arpgate>
<time value="93" pos="0" />
</arpgate>
<arpdir>
<time value="0" pos="0" />
</arpdir>
<arpmode>
<time value="0" pos="0" />
</arpmode>
</automation-pattern>
</arpandchords>
<midi>
<automation-pattern>
<inputchannel>
<time value="0" pos="0" />
</inputchannel>
<outputchannel>
<time value="1" pos="0" />
</outputchannel>
<receive>
<time value="0" pos="0" />
</receive>
<send>
<time value="0" pos="0" />
</send>
<defvelin>
<time value="0" pos="0" />
</defvelin>
<defvelout>
<time value="0" pos="0" />
</defvelout>
</automation-pattern>
</midi>
<fx fxdisabled="1" >
<rack numofeffects="0" />
</fx>
</instrumenttrack>
<pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="0" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="34" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="28" len="-64" />
<note tone="9" pan="0" oct="4" vol="176" pos="44" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="64" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="128" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="192" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="28" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="44" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="256" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="320" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="384" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="28" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="448" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="512" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="576" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="640" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="704" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="768" frozen="0" len="64" />
</track>
<track muted="0" height="32" type="0" >
<instrumenttrack width="250" x="514" y="199" height="436" name="trumpet01.ogg" tab="0" visible="0" >
<automation-pattern>
<vol>
<time value="26" pos="0" />
</vol>
<surpos-x>
<time value="0" pos="0" />
</surpos-x>
<surpos-y>
<time value="0" pos="0" />
</surpos-y>
<fxch>
<time value="0" pos="0" />
</fxch>
<basenote>
<time value="101" pos="0" />
</basenote>
</automation-pattern>
<audiofileprocessor reversed="0" looped="0" eframe="0.999947" sframe="0" amp="55" src="instruments/trumpet01.ogg" />
<eldata fwet="1" >
<automation-pattern>
<ftype>
<time value="0" pos="0" />
</ftype>
<fcut>
<time value="4480" pos="0" />
</fcut>
<fres>
<time value="1.45" pos="0" />
</fres>
</automation-pattern>
<elvol syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.486" pos="0" />
</hold>
<dec>
<time value="0.486" pos="0" />
</dec>
<sus>
<time value="0.743" pos="0" />
</sus>
<rel>
<time value="0.478" pos="0" />
</rel>
<amt>
<time value="0.895" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elvol>
<elcut syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.486" pos="0" />
</hold>
<dec>
<time value="0.486" pos="0" />
</dec>
<sus>
<time value="0.486" pos="0" />
</sus>
<rel>
<time value="0.086" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elcut>
<elres syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.486" pos="0" />
</hold>
<dec>
<time value="0.486" pos="0" />
</dec>
<sus>
<time value="0.486" pos="0" />
</sus>
<rel>
<time value="0.086" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elres>
</eldata>
<arpandchords arpdisabled="1" syncmode="0" chorddisabled="1" >
<automation-pattern>
<chord>
<time value="0" pos="0" />
</chord>
<chordrange>
<time value="1" pos="0" />
</chordrange>
<arp>
<time value="0" pos="0" />
</arp>
<arprange>
<time value="1" pos="0" />
</arprange>
<arptime>
<time value="296" pos="0" />
</arptime>
<arptime_numerator>
<time value="1" pos="0" />
</arptime_numerator>
<arptime_denominator>
<time value="1" pos="0" />
</arptime_denominator>
<arpgate>
<time value="1" pos="0" />
</arpgate>
<arpdir>
<time value="0" pos="0" />
</arpdir>
<arpmode>
<time value="0" pos="0" />
</arpmode>
</automation-pattern>
</arpandchords>
<midi>
<automation-pattern>
<inputchannel>
<time value="0" pos="0" />
</inputchannel>
<outputchannel>
<time value="1" pos="0" />
</outputchannel>
<receive>
<time value="0" pos="0" />
</receive>
<send>
<time value="0" pos="0" />
</send>
<defvelin>
<time value="0" pos="0" />
</defvelin>
<defvelout>
<time value="0" pos="0" />
</defvelout>
</automation-pattern>
</midi>
<fx fxdisabled="1" >
<rack numofeffects="0" />
</fx>
</instrumenttrack>
<pattern steps="16" muted="0" type="1" name="trumpet01.ogg" pos="0" frozen="0" len="64" >
<note tone="2" pan="0" oct="6" vol="100" pos="0" len="16" >
<automation-pattern>
<detuning>
<time value="0" pos="0" />
</detuning>
</automation-pattern>
</note>
<note tone="5" pan="0" oct="6" vol="100" pos="16" len="16" >
<automation-pattern>
<detuning>
<time value="0" pos="0" />
</detuning>
</automation-pattern>
</note>
<note tone="8" pan="0" oct="6" vol="100" pos="32" len="16" >
<automation-pattern>
<detuning>
<time value="0" pos="0" />
</detuning>
</automation-pattern>
</note>
<note tone="3" pan="0" oct="8" vol="100" pos="48" len="16" >
<automation-pattern>
<detuning>
<time value="0" pos="0" />
</detuning>
</automation-pattern>
</note>
</pattern>
<pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="64" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="128" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="192" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="28" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="256" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="320" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="384" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="448" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="512" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="576" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="640" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="704" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="768" frozen="0" len="64" />
</track>
<track muted="0" height="32" type="0" >
<instrumenttrack width="250" x="260" y="199" height="436" name="Default" tab="1" visible="0" >
<automation-pattern>
<vol>
<time value="32" pos="0" />
</vol>
<surpos-x>
<time value="1024" pos="0" />
</surpos-x>
<surpos-y>
<time value="-74" pos="0" />
</surpos-y>
<fxch>
<time value="0" pos="0" />
</fxch>
<basenote>
<time value="81" pos="0" />
</basenote>
</automation-pattern>
<tripleoscillator userwavefile1="samples/empty.wav" userwavefile2="samples/empty.wav" userwavefile0="samples/empty.wav" >
<automation-pattern>
<modalgo1>
<time value="2" pos="0" />
</modalgo1>
<modalgo2>
<time value="2" pos="0" />
</modalgo2>
<vol0>
<time value="100" pos="0" />
</vol0>
<pan0>
<time value="0" pos="0" />
</pan0>
<coarse0>
<time value="0" pos="0" />
</coarse0>
<finel0>
<time value="0" pos="0" />
</finel0>
<finer0>
<time value="0" pos="0" />
</finer0>
<phoffset0>
<time value="0" pos="0" />
</phoffset0>
<stphdetun0>
<time value="0" pos="0" />
</stphdetun0>
<wavetype0>
<time value="0" pos="0" />
</wavetype0>
<vol1>
<time value="100" pos="0" />
</vol1>
<pan1>
<time value="0" pos="0" />
</pan1>
<coarse1>
<time value="0" pos="0" />
</coarse1>
<finel1>
<time value="0" pos="0" />
</finel1>
<finer1>
<time value="0" pos="0" />
</finer1>
<phoffset1>
<time value="0" pos="0" />
</phoffset1>
<stphdetun1>
<time value="0" pos="0" />
</stphdetun1>
<wavetype1>
<time value="0" pos="0" />
</wavetype1>
<vol2>
<time value="100" pos="0" />
</vol2>
<pan2>
<time value="0" pos="0" />
</pan2>
<coarse2>
<time value="0" pos="0" />
</coarse2>
<finel2>
<time value="0" pos="0" />
</finel2>
<finer2>
<time value="0" pos="0" />
</finer2>
<phoffset2>
<time value="0" pos="0" />
</phoffset2>
<stphdetun2>
<time value="0" pos="0" />
</stphdetun2>
<wavetype2>
<time value="0" pos="0" />
</wavetype2>
</automation-pattern>
</tripleoscillator>
<eldata fwet="1" >
<automation-pattern>
<ftype>
<time value="7" pos="0" />
</ftype>
<fcut>
<time value="2560" pos="0" />
</fcut>
<fres>
<time value="2.3" pos="0" />
</fres>
</automation-pattern>
<elvol syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.157" pos="0" />
</hold>
<dec>
<time value="0.742" pos="0" />
</dec>
<sus>
<time value="0.512" pos="0" />
</sus>
<rel>
<time value="0.595" pos="0" />
</rel>
<amt>
<time value="1" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elvol>
<elcut syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.49" pos="0" />
</hold>
<dec>
<time value="0.49" pos="0" />
</dec>
<sus>
<time value="0.49" pos="0" />
</sus>
<rel>
<time value="0.09" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elcut>
<elres syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.49" pos="0" />
</hold>
<dec>
<time value="0.49" pos="0" />
</dec>
<sus>
<time value="0.49" pos="0" />
</sus>
<rel>
<time value="0.09" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elres>
</eldata>
<arpandchords arpdisabled="1" syncmode="0" chorddisabled="0" >
<automation-pattern>
<chord>
<time value="0" pos="0" />
</chord>
<chordrange>
<time value="1" pos="0" />
</chordrange>
<arp>
<time value="0" pos="0" />
</arp>
<arprange>
<time value="1" pos="0" />
</arprange>
<arptime>
<time value="100" pos="0" />
</arptime>
<arptime_numerator>
<time value="1" pos="0" />
</arptime_numerator>
<arptime_denominator>
<time value="1" pos="0" />
</arptime_denominator>
<arpgate>
<time value="100" pos="0" />
</arpgate>
<arpdir>
<time value="0" pos="0" />
</arpdir>
<arpmode>
<time value="0" pos="0" />
</arpmode>
</automation-pattern>
</arpandchords>
<midi>
<automation-pattern>
<inputchannel>
<time value="0" pos="0" />
</inputchannel>
<outputchannel>
<time value="1" pos="0" />
</outputchannel>
<receive>
<time value="0" pos="0" />
</receive>
<send>
<time value="0" pos="0" />
</send>
<defvelin>
<time value="0" pos="0" />
</defvelin>
<defvelout>
<time value="0" pos="0" />
</defvelout>
</automation-pattern>
</midi>
<fx fxdisabled="1" >
<rack numofeffects="0" />
</fx>
</instrumenttrack>
<pattern steps="16" muted="0" type="0" name="Default" pos="0" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="64" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="Default" pos="128" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="192" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="256" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="320" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="384" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="448" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="512" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="576" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="640" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="704" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="768" frozen="0" len="64" />
</track>
<track muted="0" height="32" type="0" >
<instrumenttrack width="250" x="0" y="199" height="436" name="Default" tab="1" visible="0" >
<automation-pattern>
<vol>
<time value="30" pos="0" />
</vol>
<surpos-x>
<time value="-1024" pos="0" />
</surpos-x>
<surpos-y>
<time value="-174" pos="0" />
</surpos-y>
<fxch>
<time value="0" pos="0" />
</fxch>
<basenote>
<time value="81" pos="0" />
</basenote>
</automation-pattern>
<tripleoscillator userwavefile1="samples/empty.wav" userwavefile2="samples/empty.wav" userwavefile0="samples/empty.wav" >
<automation-pattern>
<modalgo1>
<time value="2" pos="0" />
</modalgo1>
<modalgo2>
<time value="2" pos="0" />
</modalgo2>
<vol0>
<time value="100" pos="0" />
</vol0>
<pan0>
<time value="0" pos="0" />
</pan0>
<coarse0>
<time value="0" pos="0" />
</coarse0>
<finel0>
<time value="0" pos="0" />
</finel0>
<finer0>
<time value="0" pos="0" />
</finer0>
<phoffset0>
<time value="0" pos="0" />
</phoffset0>
<stphdetun0>
<time value="0" pos="0" />
</stphdetun0>
<wavetype0>
<time value="0" pos="0" />
</wavetype0>
<vol1>
<time value="100" pos="0" />
</vol1>
<pan1>
<time value="0" pos="0" />
</pan1>
<coarse1>
<time value="0" pos="0" />
</coarse1>
<finel1>
<time value="0" pos="0" />
</finel1>
<finer1>
<time value="0" pos="0" />
</finer1>
<phoffset1>
<time value="0" pos="0" />
</phoffset1>
<stphdetun1>
<time value="0" pos="0" />
</stphdetun1>
<wavetype1>
<time value="0" pos="0" />
</wavetype1>
<vol2>
<time value="100" pos="0" />
</vol2>
<pan2>
<time value="0" pos="0" />
</pan2>
<coarse2>
<time value="0" pos="0" />
</coarse2>
<finel2>
<time value="0" pos="0" />
</finel2>
<finer2>
<time value="0" pos="0" />
</finer2>
<phoffset2>
<time value="0" pos="0" />
</phoffset2>
<stphdetun2>
<time value="0" pos="0" />
</stphdetun2>
<wavetype2>
<time value="0" pos="0" />
</wavetype2>
</automation-pattern>
</tripleoscillator>
<eldata fwet="1" >
<automation-pattern>
<ftype>
<time value="7" pos="0" />
</ftype>
<fcut>
<time value="2560" pos="0" />
</fcut>
<fres>
<time value="2.01" pos="0" />
</fres>
</automation-pattern>
<elvol syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.156" pos="0" />
</hold>
<dec>
<time value="0.741" pos="0" />
</dec>
<sus>
<time value="0.512" pos="0" />
</sus>
<rel>
<time value="0.595" pos="0" />
</rel>
<amt>
<time value="1" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elvol>
<elcut syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.489" pos="0" />
</hold>
<dec>
<time value="0.489" pos="0" />
</dec>
<sus>
<time value="0.489" pos="0" />
</sus>
<rel>
<time value="0.089" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elcut>
<elres syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.489" pos="0" />
</hold>
<dec>
<time value="0.489" pos="0" />
</dec>
<sus>
<time value="0.489" pos="0" />
</sus>
<rel>
<time value="0.089" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elres>
</eldata>
<arpandchords arpdisabled="1" syncmode="0" chorddisabled="0" >
<automation-pattern>
<chord>
<time value="0" pos="0" />
</chord>
<chordrange>
<time value="1" pos="0" />
</chordrange>
<arp>
<time value="0" pos="0" />
</arp>
<arprange>
<time value="1" pos="0" />
</arprange>
<arptime>
<time value="100" pos="0" />
</arptime>
<arptime_numerator>
<time value="1" pos="0" />
</arptime_numerator>
<arptime_denominator>
<time value="1" pos="0" />
</arptime_denominator>
<arpgate>
<time value="100" pos="0" />
</arpgate>
<arpdir>
<time value="0" pos="0" />
</arpdir>
<arpmode>
<time value="0" pos="0" />
</arpmode>
</automation-pattern>
</arpandchords>
<midi>
<automation-pattern>
<inputchannel>
<time value="0" pos="0" />
</inputchannel>
<outputchannel>
<time value="1" pos="0" />
</outputchannel>
<receive>
<time value="0" pos="0" />
</receive>
<send>
<time value="0" pos="0" />
</send>
<defvelin>
<time value="0" pos="0" />
</defvelin>
<defvelout>
<time value="0" pos="0" />
</defvelout>
</automation-pattern>
</midi>
<fx fxdisabled="1" >
<rack numofeffects="0" />
</fx>
</instrumenttrack>
<pattern steps="16" muted="0" type="0" name="Default" pos="0" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="64" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="44" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="Default" pos="128" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="192" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="256" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="320" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="384" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="448" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="512" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="576" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="640" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="704" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="Default" pos="768" frozen="0" len="64" />
</track>
<track muted="0" height="32" type="0" >
<instrumenttrack width="250" x="514" y="0" height="436" name="snaph01.ogg" tab="1" visible="0" >
<automation-pattern>
<vol>
<time value="100" pos="0" />
</vol>
<surpos-x>
<time value="0" pos="0" />
</surpos-x>
<surpos-y>
<time value="0" pos="0" />
</surpos-y>
<fxch>
<time value="0" pos="0" />
</fxch>
<basenote>
<time value="57" pos="0" />
</basenote>
</automation-pattern>
<audiofileprocessor reversed="0" looped="0" eframe="0.996599" sframe="0" amp="100" src="misc/snaph01.ogg" />
<eldata fwet="1" >
<automation-pattern>
<ftype>
<time value="7" pos="0" />
</ftype>
<fcut>
<time value="4640" pos="0" />
</fcut>
<fres>
<time value="2.04" pos="0" />
</fres>
</automation-pattern>
<elvol syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.486" pos="0" />
</hold>
<dec>
<time value="0.486" pos="0" />
</dec>
<sus>
<time value="0.486" pos="0" />
</sus>
<rel>
<time value="0.086" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elvol>
<elcut syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.486" pos="0" />
</hold>
<dec>
<time value="0.486" pos="0" />
</dec>
<sus>
<time value="0.486" pos="0" />
</sus>
<rel>
<time value="0.086" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elcut>
<elres syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.486" pos="0" />
</hold>
<dec>
<time value="0.486" pos="0" />
</dec>
<sus>
<time value="0.486" pos="0" />
</sus>
<rel>
<time value="0.086" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elres>
</eldata>
<arpandchords arpdisabled="1" syncmode="0" chorddisabled="1" >
<automation-pattern>
<chord>
<time value="0" pos="0" />
</chord>
<chordrange>
<time value="1" pos="0" />
</chordrange>
<arp>
<time value="0" pos="0" />
</arp>
<arprange>
<time value="3" pos="0" />
</arprange>
<arptime>
<time value="608" pos="0" />
</arptime>
<arptime_numerator>
<time value="1" pos="0" />
</arptime_numerator>
<arptime_denominator>
<time value="1" pos="0" />
</arptime_denominator>
<arpgate>
<time value="192" pos="0" />
</arpgate>
<arpdir>
<time value="2" pos="0" />
</arpdir>
<arpmode>
<time value="0" pos="0" />
</arpmode>
</automation-pattern>
</arpandchords>
<midi>
<automation-pattern>
<inputchannel>
<time value="0" pos="0" />
</inputchannel>
<outputchannel>
<time value="1" pos="0" />
</outputchannel>
<receive>
<time value="0" pos="0" />
</receive>
<send>
<time value="0" pos="0" />
</send>
<defvelin>
<time value="0" pos="0" />
</defvelin>
<defvelout>
<time value="0" pos="0" />
</defvelout>
</automation-pattern>
</midi>
<fx fxdisabled="1" >
<rack numofeffects="0" />
</fx>
</instrumenttrack>
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="0" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="64" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="128" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="192" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="256" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="20" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="36" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="48" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="320" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="384" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="448" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="172" pos="20" len="-64" />
<note tone="9" pan="0" oct="4" vol="168" pos="24" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
<note tone="9" pan="0" oct="4" vol="122" pos="40" len="-64" />
<note tone="9" pan="0" oct="4" vol="144" pos="48" len="-64" />
<note tone="9" pan="0" oct="4" vol="200" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="512" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="576" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="640" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="704" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="20" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
<note tone="9" pan="0" oct="4" vol="98" pos="36" len="-64" />
<note tone="9" pan="0" oct="4" vol="104" pos="40" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="48" len="-64" />
<note tone="9" pan="0" oct="4" vol="102" pos="52" len="-64" />
<note tone="9" pan="0" oct="4" vol="106" pos="56" len="-64" />
<note tone="9" pan="0" oct="4" vol="104" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="768" frozen="0" len="64" />
</track>
<track muted="0" height="32" type="0" >
<instrumenttrack width="250" x="253" y="199" height="436" name="kick_soft02.ogg" tab="2" visible="0" >
<automation-pattern>
<vol>
<time value="90" pos="0" />
</vol>
<surpos-x>
<time value="0" pos="0" />
</surpos-x>
<surpos-y>
<time value="0" pos="0" />
</surpos-y>
<fxch>
<time value="0" pos="0" />
</fxch>
<basenote>
<time value="57" pos="0" />
</basenote>
</automation-pattern>
<audiofileprocessor reversed="0" looped="0" eframe="0.99946" sframe="0" amp="200" src="drums/kick_soft02.ogg" />
<eldata fwet="1" >
<automation-pattern>
<ftype>
<time value="7" pos="0" />
</ftype>
<fcut>
<time value="2720" pos="0" />
</fcut>
<fres>
<time value="0.44" pos="0" />
</fres>
</automation-pattern>
<elvol syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.99" pos="0" />
</hold>
<dec>
<time value="0.49" pos="0" />
</dec>
<sus>
<time value="0.839" pos="0" />
</sus>
<rel>
<time value="0.696" pos="0" />
</rel>
<amt>
<time value="1" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elvol>
<elcut syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.49" pos="0" />
</hold>
<dec>
<time value="0.49" pos="0" />
</dec>
<sus>
<time value="0.49" pos="0" />
</sus>
<rel>
<time value="0.99" pos="0" />
</rel>
<amt>
<time value="1" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elcut>
<elres syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.49" pos="0" />
</hold>
<dec>
<time value="0.49" pos="0" />
</dec>
<sus>
<time value="0.49" pos="0" />
</sus>
<rel>
<time value="0.09" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elres>
</eldata>
<arpandchords arpdisabled="1" syncmode="0" chorddisabled="0" >
<automation-pattern>
<chord>
<time value="0" pos="0" />
</chord>
<chordrange>
<time value="2" pos="0" />
</chordrange>
<arp>
<time value="0" pos="0" />
</arp>
<arprange>
<time value="1" pos="0" />
</arprange>
<arptime>
<time value="100" pos="0" />
</arptime>
<arptime_numerator>
<time value="1" pos="0" />
</arptime_numerator>
<arptime_denominator>
<time value="1" pos="0" />
</arptime_denominator>
<arpgate>
<time value="100" pos="0" />
</arpgate>
<arpdir>
<time value="0" pos="0" />
</arpdir>
<arpmode>
<time value="0" pos="0" />
</arpmode>
</automation-pattern>
</arpandchords>
<midi>
<automation-pattern>
<inputchannel>
<time value="0" pos="0" />
</inputchannel>
<outputchannel>
<time value="1" pos="0" />
</outputchannel>
<receive>
<time value="0" pos="0" />
</receive>
<send>
<time value="0" pos="0" />
</send>
<defvelin>
<time value="0" pos="0" />
</defvelin>
<defvelout>
<time value="0" pos="0" />
</defvelout>
</automation-pattern>
</midi>
<fx fxdisabled="1" >
<rack numofeffects="0" />
</fx>
</instrumenttrack>
<pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="0" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="64" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="128" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="158" pos="4" len="-64" />
<note tone="9" pan="0" oct="4" vol="58" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="20" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
<note tone="9" pan="0" oct="4" vol="148" pos="32" len="-64" />
<note tone="9" pan="0" oct="4" vol="154" pos="36" len="-64" />
<note tone="9" pan="0" oct="4" vol="152" pos="40" len="-64" />
<note tone="9" pan="0" oct="4" vol="186" pos="48" len="-64" />
<note tone="9" pan="0" oct="4" vol="188" pos="52" len="-64" />
<note tone="9" pan="0" oct="4" vol="188" pos="56" len="-64" />
<note tone="9" pan="0" oct="4" vol="190" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="192" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="256" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="320" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="384" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="44" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="448" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="512" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="576" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="640" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="704" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="768" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="20" len="-64" />
<note tone="9" pan="0" oct="4" vol="174" pos="24" len="-64" />
<note tone="9" pan="0" oct="4" vol="170" pos="36" len="-64" />
<note tone="9" pan="0" oct="4" vol="106" pos="40" len="-64" />
</pattern>
</track>
<track muted="0" height="32" type="0" >
<instrumenttrack width="250" x="0" y="199" height="436" name="snare03.ogg" tab="2" visible="0" >
<automation-pattern>
<vol>
<time value="28" pos="0" />
</vol>
<surpos-x>
<time value="512" pos="0" />
</surpos-x>
<surpos-y>
<time value="-853" pos="0" />
</surpos-y>
<fxch>
<time value="0" pos="0" />
</fxch>
<basenote>
<time value="57" pos="0" />
</basenote>
</automation-pattern>
<audiofileprocessor reversed="0" looped="0" eframe="0.999184" sframe="0" amp="100" src="drums/snare03.ogg" />
<eldata fwet="1" >
<automation-pattern>
<ftype>
<time value="7" pos="0" />
</ftype>
<fcut>
<time value="800" pos="0" />
</fcut>
<fres>
<time value="1.63" pos="0" />
</fres>
</automation-pattern>
<elvol syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.49" pos="0" />
</hold>
<dec>
<time value="0.49" pos="0" />
</dec>
<sus>
<time value="0.968" pos="0" />
</sus>
<rel>
<time value="0.816" pos="0" />
</rel>
<amt>
<time value="1" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elvol>
<elcut syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.49" pos="0" />
</hold>
<dec>
<time value="0.49" pos="0" />
</dec>
<sus>
<time value="0.49" pos="0" />
</sus>
<rel>
<time value="0.09" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elcut>
<elres syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.49" pos="0" />
</hold>
<dec>
<time value="0.49" pos="0" />
</dec>
<sus>
<time value="0.49" pos="0" />
</sus>
<rel>
<time value="0.09" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elres>
</eldata>
<arpandchords arpdisabled="0" syncmode="0" chorddisabled="1" >
<automation-pattern>
<chord>
<time value="0" pos="0" />
</chord>
<chordrange>
<time value="3" pos="0" />
</chordrange>
<arp>
<time value="0" pos="0" />
</arp>
<arprange>
<time value="2" pos="0" />
</arprange>
<arptime>
<time value="450" pos="0" />
</arptime>
<arptime_numerator>
<time value="1" pos="0" />
</arptime_numerator>
<arptime_denominator>
<time value="1" pos="0" />
</arptime_denominator>
<arpgate>
<time value="200" pos="0" />
</arpgate>
<arpdir>
<time value="2" pos="0" />
</arpdir>
<arpmode>
<time value="0" pos="0" />
</arpmode>
</automation-pattern>
</arpandchords>
<midi>
<automation-pattern>
<inputchannel>
<time value="0" pos="0" />
</inputchannel>
<outputchannel>
<time value="1" pos="0" />
</outputchannel>
<receive>
<time value="0" pos="0" />
</receive>
<send>
<time value="0" pos="0" />
</send>
<defvelin>
<time value="0" pos="0" />
</defvelin>
<defvelout>
<time value="0" pos="0" />
</defvelout>
</automation-pattern>
</midi>
<fx fxdisabled="1" >
<rack numofeffects="0" />
</fx>
</instrumenttrack>
<pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="0" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="64" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="128" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="138" pos="4" len="-64" />
<note tone="9" pan="0" oct="4" vol="52" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="176" pos="24" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="36" len="-64" />
<note tone="9" pan="0" oct="4" vol="162" pos="40" len="-64" />
<note tone="9" pan="0" oct="4" vol="158" pos="52" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
<note tone="9" pan="0" oct="4" vol="180" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="192" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="256" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="320" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="384" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="36" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="448" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="512" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="576" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="640" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="704" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="768" frozen="0" len="64" />
</track>
<track muted="0" height="32" type="0" >
<instrumenttrack width="250" x="513" y="199" height="436" name="wood01.ogg" tab="2" visible="0" >
<automation-pattern>
<vol>
<time value="56" pos="0" />
</vol>
<surpos-x>
<time value="0" pos="0" />
</surpos-x>
<surpos-y>
<time value="0" pos="0" />
</surpos-y>
<fxch>
<time value="0" pos="0" />
</fxch>
<basenote>
<time value="48" pos="0" />
</basenote>
</automation-pattern>
<audiofileprocessor reversed="0" looped="0" eframe="0.994691" sframe="0" amp="145" src="drums/wood01.ogg" />
<eldata fwet="1" >
<automation-pattern>
<ftype>
<time value="7" pos="0" />
</ftype>
<fcut>
<time value="2080" pos="0" />
</fcut>
<fres>
<time value="1.28" pos="0" />
</fres>
</automation-pattern>
<elvol syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.49" pos="0" />
</hold>
<dec>
<time value="0.49" pos="0" />
</dec>
<sus>
<time value="0.49" pos="0" />
</sus>
<rel>
<time value="0.09" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elvol>
<elcut syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.49" pos="0" />
</hold>
<dec>
<time value="0.49" pos="0" />
</dec>
<sus>
<time value="0.49" pos="0" />
</sus>
<rel>
<time value="0.09" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elcut>
<elres syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.49" pos="0" />
</hold>
<dec>
<time value="0.49" pos="0" />
</dec>
<sus>
<time value="0.49" pos="0" />
</sus>
<rel>
<time value="0.09" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elres>
</eldata>
<arpandchords arpdisabled="1" syncmode="0" chorddisabled="1" >
<automation-pattern>
<chord>
<time value="0" pos="0" />
</chord>
<chordrange>
<time value="1" pos="0" />
</chordrange>
<arp>
<time value="0" pos="0" />
</arp>
<arprange>
<time value="4" pos="0" />
</arprange>
<arptime>
<time value="888" pos="0" />
</arptime>
<arptime_numerator>
<time value="1" pos="0" />
</arptime_numerator>
<arptime_denominator>
<time value="1" pos="0" />
</arptime_denominator>
<arpgate>
<time value="200" pos="0" />
</arpgate>
<arpdir>
<time value="0" pos="0" />
</arpdir>
<arpmode>
<time value="0" pos="0" />
</arpmode>
</automation-pattern>
</arpandchords>
<midi>
<automation-pattern>
<inputchannel>
<time value="0" pos="0" />
</inputchannel>
<outputchannel>
<time value="1" pos="0" />
</outputchannel>
<receive>
<time value="0" pos="0" />
</receive>
<send>
<time value="0" pos="0" />
</send>
<defvelin>
<time value="0" pos="0" />
</defvelin>
<defvelout>
<time value="0" pos="0" />
</defvelout>
</automation-pattern>
</midi>
<fx fxdisabled="1" >
<rack numofeffects="0" />
</fx>
</instrumenttrack>
<pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="0" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="64" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="128" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="192" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="256" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="320" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="40" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="384" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="448" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="512" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="576" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
<note tone="9" pan="0" oct="4" vol="58" pos="8" len="-64" />
<note tone="9" pan="0" oct="4" vol="176" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="20" len="-64" />
<note tone="9" pan="0" oct="4" vol="60" pos="24" len="-64" />
<note tone="9" pan="0" oct="4" vol="170" pos="28" len="-64" />
<note tone="9" pan="0" oct="4" vol="108" pos="40" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
<note tone="9" pan="0" oct="4" vol="200" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="640" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="20" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="36" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="40" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="704" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="20" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="36" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="40" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="48" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="768" frozen="0" len="64" />
</track>
<track muted="0" height="32" type="0" >
<instrumenttrack width="250" x="260" y="0" height="436" name="snaph01.ogg" tab="1" visible="0" >
<automation-pattern>
<vol>
<time value="200" pos="0" />
</vol>
<surpos-x>
<time value="0" pos="0" />
</surpos-x>
<surpos-y>
<time value="0" pos="0" />
</surpos-y>
<fxch>
<time value="0" pos="0" />
</fxch>
<basenote>
<time value="57" pos="0" />
</basenote>
</automation-pattern>
<audiofileprocessor reversed="0" looped="0" eframe="0.996473" sframe="0" amp="120" src="misc/snaph01.ogg" />
<eldata fwet="1" >
<automation-pattern>
<ftype>
<time value="7" pos="0" />
</ftype>
<fcut>
<time value="640" pos="0" />
</fcut>
<fres>
<time value="10" pos="0" />
</fres>
</automation-pattern>
<elvol syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.581" pos="0" />
</hold>
<dec>
<time value="0.485" pos="0" />
</dec>
<sus>
<time value="0.211" pos="0" />
</sus>
<rel>
<time value="0.152" pos="0" />
</rel>
<amt>
<time value="0.895" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0.162" pos="0" />
</latt>
<lspd>
<time value="0.1384" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="1" pos="0" />
</lamt>
<x100>
<time value="1" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elvol>
<elcut syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0.077" pos="0" />
</att>
<hold>
<time value="0.558" pos="0" />
</hold>
<dec>
<time value="0.485" pos="0" />
</dec>
<sus>
<time value="0.544" pos="0" />
</sus>
<rel>
<time value="0.434" pos="0" />
</rel>
<amt>
<time value="-0.295" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elcut>
<elres syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.485" pos="0" />
</hold>
<dec>
<time value="0.485" pos="0" />
</dec>
<sus>
<time value="0.798" pos="0" />
</sus>
<rel>
<time value="0.085" pos="0" />
</rel>
<amt>
<time value="0.64" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elres>
</eldata>
<arpandchords arpdisabled="1" syncmode="0" chorddisabled="1" >
<automation-pattern>
<chord>
<time value="0" pos="0" />
</chord>
<chordrange>
<time value="4" pos="0" />
</chordrange>
<arp>
<time value="0" pos="0" />
</arp>
<arprange>
<time value="3" pos="0" />
</arprange>
<arptime>
<time value="608" pos="0" />
</arptime>
<arptime_numerator>
<time value="1" pos="0" />
</arptime_numerator>
<arptime_denominator>
<time value="1" pos="0" />
</arptime_denominator>
<arpgate>
<time value="192" pos="0" />
</arpgate>
<arpdir>
<time value="2" pos="0" />
</arpdir>
<arpmode>
<time value="0" pos="0" />
</arpmode>
</automation-pattern>
</arpandchords>
<midi>
<automation-pattern>
<inputchannel>
<time value="0" pos="0" />
</inputchannel>
<outputchannel>
<time value="1" pos="0" />
</outputchannel>
<receive>
<time value="0" pos="0" />
</receive>
<send>
<time value="0" pos="0" />
</send>
<defvelin>
<time value="0" pos="0" />
</defvelin>
<defvelout>
<time value="0" pos="0" />
</defvelout>
</automation-pattern>
</midi>
<fx fxdisabled="1" >
<rack numofeffects="0" />
</fx>
</instrumenttrack>
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="0" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="64" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="128" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="192" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="256" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="320" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="384" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="448" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="512" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="40" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="576" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="640" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="704" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="768" frozen="0" len="64" />
</track>
<track muted="0" height="32" type="0" >
<instrumenttrack width="250" x="514" y="0" height="436" name="tom05.ogg" tab="1" visible="0" >
<automation-pattern>
<vol>
<time value="100" pos="0" />
</vol>
<surpos-x>
<time value="0" pos="0" />
</surpos-x>
<surpos-y>
<time value="0" pos="0" />
</surpos-y>
<fxch>
<time value="0" pos="0" />
</fxch>
<basenote>
<time value="57" pos="0" />
</basenote>
</automation-pattern>
<audiofileprocessor reversed="0" looped="0" eframe="0.999726" sframe="0" amp="100" src="drums/tom05.ogg" />
<eldata fwet="1" >
<automation-pattern>
<ftype>
<time value="7" pos="0" />
</ftype>
<fcut>
<time value="160" pos="0" />
</fcut>
<fres>
<time value="2.81" pos="0" />
</fres>
</automation-pattern>
<elvol syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.495" pos="0" />
</hold>
<dec>
<time value="0.495" pos="0" />
</dec>
<sus>
<time value="0.495" pos="0" />
</sus>
<rel>
<time value="0.095" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elvol>
<elcut syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0" pos="0" />
</att>
<hold>
<time value="0.495" pos="0" />
</hold>
<dec>
<time value="0.495" pos="0" />
</dec>
<sus>
<time value="0.495" pos="0" />
</sus>
<rel>
<time value="0.095" pos="0" />
</rel>
<amt>
<time value="0" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elcut>
<elres syncmode="0" userwavefile="" >
<automation-pattern>
<pdel>
<time value="0" pos="0" />
</pdel>
<att>
<time value="0.128" pos="0" />
</att>
<hold>
<time value="0.687" pos="0" />
</hold>
<dec>
<time value="0.495" pos="0" />
</dec>
<sus>
<time value="0.683" pos="0" />
</sus>
<rel>
<time value="0.095" pos="0" />
</rel>
<amt>
<time value="0.51" pos="0" />
</amt>
<lshp>
<time value="0" pos="0" />
</lshp>
<lpdel>
<time value="0" pos="0" />
</lpdel>
<latt>
<time value="0" pos="0" />
</latt>
<lspd>
<time value="0.1" pos="0" />
</lspd>
<lspd_numerator>
<time value="1" pos="0" />
</lspd_numerator>
<lspd_denominator>
<time value="1" pos="0" />
</lspd_denominator>
<lamt>
<time value="0.01" pos="0" />
</lamt>
<x100>
<time value="0" pos="0" />
</x100>
<ctlenvamt>
<time value="0" pos="0" />
</ctlenvamt>
</automation-pattern>
</elres>
</eldata>
<arpandchords arpdisabled="1" syncmode="0" chorddisabled="1" >
<automation-pattern>
<chord>
<time value="0" pos="0" />
</chord>
<chordrange>
<time value="1" pos="0" />
</chordrange>
<arp>
<time value="0" pos="0" />
</arp>
<arprange>
<time value="1" pos="0" />
</arprange>
<arptime>
<time value="100" pos="0" />
</arptime>
<arptime_numerator>
<time value="1" pos="0" />
</arptime_numerator>
<arptime_denominator>
<time value="1" pos="0" />
</arptime_denominator>
<arpgate>
<time value="100" pos="0" />
</arpgate>
<arpdir>
<time value="0" pos="0" />
</arpdir>
<arpmode>
<time value="0" pos="0" />
</arpmode>
</automation-pattern>
</arpandchords>
<midi>
<automation-pattern>
<inputchannel>
<time value="0" pos="0" />
</inputchannel>
<outputchannel>
<time value="1" pos="0" />
</outputchannel>
<receive>
<time value="0" pos="0" />
</receive>
<send>
<time value="0" pos="0" />
</send>
<defvelin>
<time value="0" pos="0" />
</defvelin>
<defvelout>
<time value="0" pos="0" />
</defvelout>
</automation-pattern>
</midi>
<fx fxdisabled="1" >
<rack numofeffects="0" />
</fx>
</instrumenttrack>
<pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="0" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="64" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="128" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="192" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="256" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="320" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="384" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="448" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="512" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="576" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="640" frozen="0" len="64" >
<note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="28" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="36" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="40" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
<note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
</pattern>
<pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="704" frozen="0" len="64" />
<pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="768" frozen="0" len="64" />
</track>
</trackcontainer>
</bbtrack>
<bbtco muted="0" name="start" color="4282417407" pos="256" len="64" />
<bbtco muted="0" name="start" color="4282417407" pos="4352" len="64" />
<bbtco muted="0" name="start" color="4282417407" pos="6144" len="64" />
<bbtco muted="0" name="start" color="4282417407" pos="2304" len="64" />
<bbtco muted="0" name="start" color="4282417407" pos="8448" len="64" />
</track>
<track muted="0" height="32" type="1" >
<bbtrack icon="" name="hrrrrrrrrrr" />
<bbtco muted="0" name="hrrrrrrrrrr" color="4282417407" pos="0" len="768" />
<bbtco muted="0" name="hrrrrrrrrrr" color="4282417407" pos="2048" len="764" />
<bbtco muted="0" name="hrrrrrrrrrr" color="4282417407" pos="5888" len="2048" />
<bbtco muted="0" name="hrrrrrrrrrr" color="4282417407" pos="4096" len="764" />
<bbtco muted="0" name="hrrrrrrrrrr" color="4282417407" pos="8192" len="260" />
</track>
<track muted="0" height="32" type="1" >
<bbtrack icon="" name="trrrrrrrrrrrrr" />
<bbtco muted="0" name="trrrrrrrrrrrrr" color="4282417407" pos="2240" len="192" />
<bbtco muted="0" name="trrrrrrrrrrrrr" color="4282417407" pos="6144" len="64" />
</track>
<track muted="0" height="32" type="1" >
<bbtrack icon="" name="beat1" />
<bbtco muted="0" name="beat1" color="4282417407" pos="256" len="2044" />
<bbtco muted="0" name="beat1" color="4282417407" pos="4352" len="4092" />
</track>
<track muted="0" height="32" type="1" >
<bbtrack icon="" name="first lap snap" />
<bbtco muted="0" name="first lap snap" color="4282417407" pos="252" len="1024" />
<bbtco muted="0" name="first lap snap" color="4282417407" pos="4612" len="248" />
<bbtco muted="0" name="first lap snap" color="4282417407" pos="5120" len="256" />
<bbtco muted="0" name="first lap snap" color="4282417407" pos="5632" len="252" />
<bbtco muted="0" name="first lap snap" color="4282417407" pos="7680" len="256" />
</track>
<track muted="0" height="32" type="1" >
<bbtrack icon="" name="fist lap wood" />
<bbtco muted="0" name="fist lap wood" color="4282417407" pos="1280" len="1020" />
<bbtco muted="0" name="fist lap wood" color="4282417407" pos="7424" len="256" />
</track>
<track muted="0" height="32" type="1" >
<bbtrack icon="" name="beat2" />
<bbtco muted="0" name="beat2" color="4282417407" pos="2304" len="2048" />
</track>
<track muted="0" height="32" type="1" >
<bbtrack icon="" name="second lap snap" />
<bbtco muted="0" name="first lap snap" color="4282417407" pos="2304" len="1024" />
<bbtco muted="0" name="second lap snap" color="4282417407" pos="4864" len="252" />
<bbtco muted="0" name="second lap snap" color="4282417407" pos="5632" len="512" />
<bbtco muted="0" name="second lap snap" color="4282417407" pos="7168" len="256" />
</track>
<track muted="0" height="32" type="1" >
<bbtrack icon="" name="third lap snap" />
<bbtco muted="0" name="third lap snap" color="4282417407" pos="4352" len="1016" />
<bbtco muted="0" name="third lap snap" color="4282417407" pos="6656" len="256" />
</track>
<track muted="0" height="32" type="1" >
<bbtrack icon="" name="second lap wood" />
<bbtco muted="0" name="fist lap wood" color="4282417407" pos="3328" len="1024" />
<bbtco muted="0" name="second lap wood" color="4282417407" pos="6912" len="256" />
</track>
<track muted="0" height="32" type="1" >
<bbtrack icon="" name="third lap wood" />
<bbtco muted="0" name="third lap wood" color="4282417407" pos="5120" len="1536" />
</track>
<track muted="0" height="32" type="1" >
<bbtrack icon="" name="final" />
<bbtco muted="0" name="final" color="4282417407" pos="7932" len="512" />
</track>
<track muted="0" height="32" type="1" >
<bbtrack icon="" name="final beat" />
<bbtco muted="0" name="final beat" color="4282417407" pos="6144" len="2048" />
</track>
</trackcontainer>
<pianoroll width="640" x="0" y="0" height="480" visible="0" />
<automation-editor width="640" x="0" y="0" height="480" visible="0" />
<projectnotes width="300" x="0" y="197" height="200" visible="1" ><![CDATA[<html><head><meta name="qrichtext" content="1" /></head><body style="font-size:10pt;font-family:Sans Serif">
<p>license:GPL version2</p>
<p>A race betwin instruments. :)</p>
<p>(c)  zvonsully@gmail.com 2006 </p>
</body></html>
]]></projectnotes>
<timeline lp1pos="64" lp0pos="0" lpstate="0" />
</song>
</multimediaproject>
