<?xml version="1.0"?>
<!DOCTYPE multimedia-project>
<multimediaproject creator="Linux MultiMedia Studio (LMMS)" creatorversion="0.2.1-svn20070228" type="song" version="1.0" >
 <head>
  <automation-pattern>
   <bpm>
    <time value="140" pos="0" />
   </bpm>
   <mastervol>
    <time value="20" pos="0" />
   </mastervol>
   <masterpitch>
    <time value="0" pos="0" />
   </masterpitch>
  </automation-pattern>
 </head>
 <song>
  <trackcontainer width="748" x="160" y="15" height="503" type="songeditor" visible="1" >
   <track muted="0" height="32" type="1" >
    <bbtrack icon="" name="start of lap" >
     <trackcontainer width="504" x="194" y="214" height="300" type="bbeditor" visible="1" >
      <track muted="0" height="32" type="0" >
       <instrumenttrack width="250" x="514" y="199" height="436" name="bassdrum02.ogg" tab="1" visible="0" >
        <automation-pattern>
         <vol>
          <time value="200" pos="0" />
         </vol>
         <surpos-x>
          <time value="0" pos="0" />
         </surpos-x>
         <surpos-y>
          <time value="0" pos="0" />
         </surpos-y>
         <fxch>
          <time value="0" pos="0" />
         </fxch>
         <basenote>
          <time value="57" pos="0" />
         </basenote>
        </automation-pattern>
        <audiofileprocessor reversed="0" looped="0" eframe="0.997757" sframe="0" amp="130" src="drums/bassdrum02.ogg" />
        <eldata fwet="1" >
         <automation-pattern>
          <ftype>
           <time value="7" pos="0" />
          </ftype>
          <fcut>
           <time value="2560" pos="0" />
          </fcut>
          <fres>
           <time value="0.69" pos="0" />
          </fres>
         </automation-pattern>
         <elvol syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.992" pos="0" />
           </hold>
           <dec>
            <time value="0.2" pos="0" />
           </dec>
           <sus>
            <time value="0.679" pos="0" />
           </sus>
           <rel>
            <time value="0.924" pos="0" />
           </rel>
           <amt>
            <time value="1" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elvol>
         <elcut syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0.392" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.938" pos="0" />
           </hold>
           <dec>
            <time value="0.479" pos="0" />
           </dec>
           <sus>
            <time value="0.479" pos="0" />
           </sus>
           <rel>
            <time value="0.355" pos="0" />
           </rel>
           <amt>
            <time value="-0.195" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elcut>
         <elres syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0.035" pos="0" />
           </att>
           <hold>
            <time value="0.892" pos="0" />
           </hold>
           <dec>
            <time value="0.479" pos="0" />
           </dec>
           <sus>
            <time value="0.544" pos="0" />
           </sus>
           <rel>
            <time value="0.61" pos="0" />
           </rel>
           <amt>
            <time value="1" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elres>
        </eldata>
        <arpandchords arpdisabled="1" syncmode="0" chorddisabled="1" >
         <automation-pattern>
          <chord>
           <time value="0" pos="0" />
          </chord>
          <chordrange>
           <time value="2" pos="0" />
          </chordrange>
          <arp>
           <time value="0" pos="0" />
          </arp>
          <arprange>
           <time value="1" pos="0" />
          </arprange>
          <arptime>
           <time value="1000" pos="0" />
          </arptime>
          <arptime_numerator>
           <time value="1" pos="0" />
          </arptime_numerator>
          <arptime_denominator>
           <time value="1" pos="0" />
          </arptime_denominator>
          <arpgate>
           <time value="93" pos="0" />
          </arpgate>
          <arpdir>
           <time value="0" pos="0" />
          </arpdir>
          <arpmode>
           <time value="0" pos="0" />
          </arpmode>
         </automation-pattern>
        </arpandchords>
        <midi>
         <automation-pattern>
          <inputchannel>
           <time value="0" pos="0" />
          </inputchannel>
          <outputchannel>
           <time value="1" pos="0" />
          </outputchannel>
          <receive>
           <time value="0" pos="0" />
          </receive>
          <send>
           <time value="0" pos="0" />
          </send>
          <defvelin>
           <time value="0" pos="0" />
          </defvelin>
          <defvelout>
           <time value="0" pos="0" />
          </defvelout>
         </automation-pattern>
        </midi>
        <fx fxdisabled="1" >
         <rack numofeffects="0" />
        </fx>
       </instrumenttrack>
       <pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="0" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="34" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="28" len="-64" />
        <note tone="9" pan="0" oct="4" vol="176" pos="44" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="64" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="128" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="192" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="28" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="44" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="256" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="320" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="384" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="28" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="448" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="512" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="576" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="640" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="704" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="bassdrum02.ogg" pos="768" frozen="0" len="64" />
      </track>
      <track muted="0" height="32" type="0" >
       <instrumenttrack width="250" x="514" y="199" height="436" name="trumpet01.ogg" tab="0" visible="0" >
        <automation-pattern>
         <vol>
          <time value="26" pos="0" />
         </vol>
         <surpos-x>
          <time value="0" pos="0" />
         </surpos-x>
         <surpos-y>
          <time value="0" pos="0" />
         </surpos-y>
         <fxch>
          <time value="0" pos="0" />
         </fxch>
         <basenote>
          <time value="101" pos="0" />
         </basenote>
        </automation-pattern>
        <audiofileprocessor reversed="0" looped="0" eframe="0.999932" sframe="0" amp="55" src="instruments/trumpet01.ogg" />
        <eldata fwet="1" >
         <automation-pattern>
          <ftype>
           <time value="0" pos="0" />
          </ftype>
          <fcut>
           <time value="4480" pos="0" />
          </fcut>
          <fres>
           <time value="1.45" pos="0" />
          </fres>
         </automation-pattern>
         <elvol syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.486" pos="0" />
           </hold>
           <dec>
            <time value="0.486" pos="0" />
           </dec>
           <sus>
            <time value="0.743" pos="0" />
           </sus>
           <rel>
            <time value="0.478" pos="0" />
           </rel>
           <amt>
            <time value="0.895" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elvol>
         <elcut syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.486" pos="0" />
           </hold>
           <dec>
            <time value="0.486" pos="0" />
           </dec>
           <sus>
            <time value="0.486" pos="0" />
           </sus>
           <rel>
            <time value="0.086" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elcut>
         <elres syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.486" pos="0" />
           </hold>
           <dec>
            <time value="0.486" pos="0" />
           </dec>
           <sus>
            <time value="0.486" pos="0" />
           </sus>
           <rel>
            <time value="0.086" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elres>
        </eldata>
        <arpandchords arpdisabled="1" syncmode="0" chorddisabled="1" >
         <automation-pattern>
          <chord>
           <time value="0" pos="0" />
          </chord>
          <chordrange>
           <time value="1" pos="0" />
          </chordrange>
          <arp>
           <time value="0" pos="0" />
          </arp>
          <arprange>
           <time value="1" pos="0" />
          </arprange>
          <arptime>
           <time value="296" pos="0" />
          </arptime>
          <arptime_numerator>
           <time value="1" pos="0" />
          </arptime_numerator>
          <arptime_denominator>
           <time value="1" pos="0" />
          </arptime_denominator>
          <arpgate>
           <time value="1" pos="0" />
          </arpgate>
          <arpdir>
           <time value="0" pos="0" />
          </arpdir>
          <arpmode>
           <time value="0" pos="0" />
          </arpmode>
         </automation-pattern>
        </arpandchords>
        <midi>
         <automation-pattern>
          <inputchannel>
           <time value="0" pos="0" />
          </inputchannel>
          <outputchannel>
           <time value="1" pos="0" />
          </outputchannel>
          <receive>
           <time value="0" pos="0" />
          </receive>
          <send>
           <time value="0" pos="0" />
          </send>
          <defvelin>
           <time value="0" pos="0" />
          </defvelin>
          <defvelout>
           <time value="0" pos="0" />
          </defvelout>
         </automation-pattern>
        </midi>
        <fx fxdisabled="1" >
         <rack numofeffects="0" />
        </fx>
       </instrumenttrack>
       <pattern steps="16" muted="0" type="1" name="trumpet01.ogg" pos="0" frozen="0" len="64" >
        <note tone="2" pan="0" oct="6" vol="100" pos="0" len="16" >
         <automation-pattern>
          <detuning>
           <time value="0" pos="0" />
          </detuning>
         </automation-pattern>
        </note>
        <note tone="5" pan="0" oct="6" vol="100" pos="16" len="16" >
         <automation-pattern>
          <detuning>
           <time value="0" pos="0" />
          </detuning>
         </automation-pattern>
        </note>
        <note tone="8" pan="0" oct="6" vol="100" pos="32" len="16" >
         <automation-pattern>
          <detuning>
           <time value="0" pos="0" />
          </detuning>
         </automation-pattern>
        </note>
        <note tone="3" pan="0" oct="8" vol="100" pos="48" len="16" >
         <automation-pattern>
          <detuning>
           <time value="0" pos="0" />
          </detuning>
         </automation-pattern>
        </note>
       </pattern>
       <pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="64" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="128" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="192" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="28" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="256" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="320" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="384" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="448" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="512" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="576" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="640" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="704" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="trumpet01.ogg" pos="768" frozen="0" len="64" />
      </track>
      <track muted="0" height="32" type="0" >
       <instrumenttrack width="250" x="260" y="199" height="436" name="Default" tab="1" visible="0" >
        <automation-pattern>
         <vol>
          <time value="32" pos="0" />
         </vol>
         <surpos-x>
          <time value="1024" pos="0" />
         </surpos-x>
         <surpos-y>
          <time value="-74" pos="0" />
         </surpos-y>
         <fxch>
          <time value="0" pos="0" />
         </fxch>
         <basenote>
          <time value="81" pos="0" />
         </basenote>
        </automation-pattern>
        <tripleoscillator userwavefile1="samples/empty.wav" userwavefile2="samples/empty.wav" userwavefile0="samples/empty.wav" >
         <automation-pattern>
          <modalgo1>
           <time value="2" pos="0" />
          </modalgo1>
          <modalgo2>
           <time value="2" pos="0" />
          </modalgo2>
          <vol0>
           <time value="100" pos="0" />
          </vol0>
          <pan0>
           <time value="0" pos="0" />
          </pan0>
          <coarse0>
           <time value="0" pos="0" />
          </coarse0>
          <finel0>
           <time value="0" pos="0" />
          </finel0>
          <finer0>
           <time value="0" pos="0" />
          </finer0>
          <phoffset0>
           <time value="0" pos="0" />
          </phoffset0>
          <stphdetun0>
           <time value="0" pos="0" />
          </stphdetun0>
          <wavetype0>
           <time value="0" pos="0" />
          </wavetype0>
          <vol1>
           <time value="100" pos="0" />
          </vol1>
          <pan1>
           <time value="0" pos="0" />
          </pan1>
          <coarse1>
           <time value="0" pos="0" />
          </coarse1>
          <finel1>
           <time value="0" pos="0" />
          </finel1>
          <finer1>
           <time value="0" pos="0" />
          </finer1>
          <phoffset1>
           <time value="0" pos="0" />
          </phoffset1>
          <stphdetun1>
           <time value="0" pos="0" />
          </stphdetun1>
          <wavetype1>
           <time value="0" pos="0" />
          </wavetype1>
          <vol2>
           <time value="100" pos="0" />
          </vol2>
          <pan2>
           <time value="0" pos="0" />
          </pan2>
          <coarse2>
           <time value="0" pos="0" />
          </coarse2>
          <finel2>
           <time value="0" pos="0" />
          </finel2>
          <finer2>
           <time value="0" pos="0" />
          </finer2>
          <phoffset2>
           <time value="0" pos="0" />
          </phoffset2>
          <stphdetun2>
           <time value="0" pos="0" />
          </stphdetun2>
          <wavetype2>
           <time value="0" pos="0" />
          </wavetype2>
         </automation-pattern>
        </tripleoscillator>
        <eldata fwet="1" >
         <automation-pattern>
          <ftype>
           <time value="7" pos="0" />
          </ftype>
          <fcut>
           <time value="2560" pos="0" />
          </fcut>
          <fres>
           <time value="2.3" pos="0" />
          </fres>
         </automation-pattern>
         <elvol syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.157" pos="0" />
           </hold>
           <dec>
            <time value="0.742" pos="0" />
           </dec>
           <sus>
            <time value="0.512" pos="0" />
           </sus>
           <rel>
            <time value="0.595" pos="0" />
           </rel>
           <amt>
            <time value="1" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elvol>
         <elcut syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.49" pos="0" />
           </hold>
           <dec>
            <time value="0.49" pos="0" />
           </dec>
           <sus>
            <time value="0.49" pos="0" />
           </sus>
           <rel>
            <time value="0.09" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elcut>
         <elres syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.49" pos="0" />
           </hold>
           <dec>
            <time value="0.49" pos="0" />
           </dec>
           <sus>
            <time value="0.49" pos="0" />
           </sus>
           <rel>
            <time value="0.09" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elres>
        </eldata>
        <arpandchords arpdisabled="1" syncmode="0" chorddisabled="0" >
         <automation-pattern>
          <chord>
           <time value="0" pos="0" />
          </chord>
          <chordrange>
           <time value="1" pos="0" />
          </chordrange>
          <arp>
           <time value="0" pos="0" />
          </arp>
          <arprange>
           <time value="1" pos="0" />
          </arprange>
          <arptime>
           <time value="100" pos="0" />
          </arptime>
          <arptime_numerator>
           <time value="1" pos="0" />
          </arptime_numerator>
          <arptime_denominator>
           <time value="1" pos="0" />
          </arptime_denominator>
          <arpgate>
           <time value="100" pos="0" />
          </arpgate>
          <arpdir>
           <time value="0" pos="0" />
          </arpdir>
          <arpmode>
           <time value="0" pos="0" />
          </arpmode>
         </automation-pattern>
        </arpandchords>
        <midi>
         <automation-pattern>
          <inputchannel>
           <time value="0" pos="0" />
          </inputchannel>
          <outputchannel>
           <time value="1" pos="0" />
          </outputchannel>
          <receive>
           <time value="0" pos="0" />
          </receive>
          <send>
           <time value="0" pos="0" />
          </send>
          <defvelin>
           <time value="0" pos="0" />
          </defvelin>
          <defvelout>
           <time value="0" pos="0" />
          </defvelout>
         </automation-pattern>
        </midi>
        <fx fxdisabled="1" >
         <rack numofeffects="0" />
        </fx>
       </instrumenttrack>
       <pattern steps="16" muted="0" type="0" name="Default" pos="0" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="64" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="Default" pos="128" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="192" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="256" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="320" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="384" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="448" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="512" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="576" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="640" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="704" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="768" frozen="0" len="64" />
      </track>
      <track muted="0" height="32" type="0" >
       <instrumenttrack width="250" x="0" y="199" height="436" name="Default" tab="1" visible="0" >
        <automation-pattern>
         <vol>
          <time value="30" pos="0" />
         </vol>
         <surpos-x>
          <time value="-1024" pos="0" />
         </surpos-x>
         <surpos-y>
          <time value="-174" pos="0" />
         </surpos-y>
         <fxch>
          <time value="0" pos="0" />
         </fxch>
         <basenote>
          <time value="81" pos="0" />
         </basenote>
        </automation-pattern>
        <tripleoscillator userwavefile1="samples/empty.wav" userwavefile2="samples/empty.wav" userwavefile0="samples/empty.wav" >
         <automation-pattern>
          <modalgo1>
           <time value="2" pos="0" />
          </modalgo1>
          <modalgo2>
           <time value="2" pos="0" />
          </modalgo2>
          <vol0>
           <time value="100" pos="0" />
          </vol0>
          <pan0>
           <time value="0" pos="0" />
          </pan0>
          <coarse0>
           <time value="0" pos="0" />
          </coarse0>
          <finel0>
           <time value="0" pos="0" />
          </finel0>
          <finer0>
           <time value="0" pos="0" />
          </finer0>
          <phoffset0>
           <time value="0" pos="0" />
          </phoffset0>
          <stphdetun0>
           <time value="0" pos="0" />
          </stphdetun0>
          <wavetype0>
           <time value="0" pos="0" />
          </wavetype0>
          <vol1>
           <time value="100" pos="0" />
          </vol1>
          <pan1>
           <time value="0" pos="0" />
          </pan1>
          <coarse1>
           <time value="0" pos="0" />
          </coarse1>
          <finel1>
           <time value="0" pos="0" />
          </finel1>
          <finer1>
           <time value="0" pos="0" />
          </finer1>
          <phoffset1>
           <time value="0" pos="0" />
          </phoffset1>
          <stphdetun1>
           <time value="0" pos="0" />
          </stphdetun1>
          <wavetype1>
           <time value="0" pos="0" />
          </wavetype1>
          <vol2>
           <time value="100" pos="0" />
          </vol2>
          <pan2>
           <time value="0" pos="0" />
          </pan2>
          <coarse2>
           <time value="0" pos="0" />
          </coarse2>
          <finel2>
           <time value="0" pos="0" />
          </finel2>
          <finer2>
           <time value="0" pos="0" />
          </finer2>
          <phoffset2>
           <time value="0" pos="0" />
          </phoffset2>
          <stphdetun2>
           <time value="0" pos="0" />
          </stphdetun2>
          <wavetype2>
           <time value="0" pos="0" />
          </wavetype2>
         </automation-pattern>
        </tripleoscillator>
        <eldata fwet="1" >
         <automation-pattern>
          <ftype>
           <time value="7" pos="0" />
          </ftype>
          <fcut>
           <time value="2560" pos="0" />
          </fcut>
          <fres>
           <time value="2.01" pos="0" />
          </fres>
         </automation-pattern>
         <elvol syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.156" pos="0" />
           </hold>
           <dec>
            <time value="0.741" pos="0" />
           </dec>
           <sus>
            <time value="0.512" pos="0" />
           </sus>
           <rel>
            <time value="0.595" pos="0" />
           </rel>
           <amt>
            <time value="1" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elvol>
         <elcut syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.489" pos="0" />
           </hold>
           <dec>
            <time value="0.489" pos="0" />
           </dec>
           <sus>
            <time value="0.489" pos="0" />
           </sus>
           <rel>
            <time value="0.089" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elcut>
         <elres syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.489" pos="0" />
           </hold>
           <dec>
            <time value="0.489" pos="0" />
           </dec>
           <sus>
            <time value="0.489" pos="0" />
           </sus>
           <rel>
            <time value="0.089" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elres>
        </eldata>
        <arpandchords arpdisabled="1" syncmode="0" chorddisabled="0" >
         <automation-pattern>
          <chord>
           <time value="0" pos="0" />
          </chord>
          <chordrange>
           <time value="1" pos="0" />
          </chordrange>
          <arp>
           <time value="0" pos="0" />
          </arp>
          <arprange>
           <time value="1" pos="0" />
          </arprange>
          <arptime>
           <time value="100" pos="0" />
          </arptime>
          <arptime_numerator>
           <time value="1" pos="0" />
          </arptime_numerator>
          <arptime_denominator>
           <time value="1" pos="0" />
          </arptime_denominator>
          <arpgate>
           <time value="100" pos="0" />
          </arpgate>
          <arpdir>
           <time value="0" pos="0" />
          </arpdir>
          <arpmode>
           <time value="0" pos="0" />
          </arpmode>
         </automation-pattern>
        </arpandchords>
        <midi>
         <automation-pattern>
          <inputchannel>
           <time value="0" pos="0" />
          </inputchannel>
          <outputchannel>
           <time value="1" pos="0" />
          </outputchannel>
          <receive>
           <time value="0" pos="0" />
          </receive>
          <send>
           <time value="0" pos="0" />
          </send>
          <defvelin>
           <time value="0" pos="0" />
          </defvelin>
          <defvelout>
           <time value="0" pos="0" />
          </defvelout>
         </automation-pattern>
        </midi>
        <fx fxdisabled="1" >
         <rack numofeffects="0" />
        </fx>
       </instrumenttrack>
       <pattern steps="16" muted="0" type="0" name="Default" pos="0" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="64" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="44" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="Default" pos="128" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="192" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="256" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="320" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="384" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="448" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="512" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="576" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="640" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="704" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="Default" pos="768" frozen="0" len="64" />
      </track>
      <track muted="0" height="32" type="0" >
       <instrumenttrack width="250" x="514" y="0" height="436" name="snaph01.ogg" tab="1" visible="0" >
        <automation-pattern>
         <vol>
          <time value="100" pos="0" />
         </vol>
         <surpos-x>
          <time value="0" pos="0" />
         </surpos-x>
         <surpos-y>
          <time value="0" pos="0" />
         </surpos-y>
         <fxch>
          <time value="0" pos="0" />
         </fxch>
         <basenote>
          <time value="57" pos="0" />
         </basenote>
        </automation-pattern>
        <audiofileprocessor reversed="0" looped="0" eframe="0.996473" sframe="0" amp="100" src="misc/snaph01.ogg" />
        <eldata fwet="1" >
         <automation-pattern>
          <ftype>
           <time value="7" pos="0" />
          </ftype>
          <fcut>
           <time value="4640" pos="0" />
          </fcut>
          <fres>
           <time value="2.04" pos="0" />
          </fres>
         </automation-pattern>
         <elvol syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.486" pos="0" />
           </hold>
           <dec>
            <time value="0.486" pos="0" />
           </dec>
           <sus>
            <time value="0.486" pos="0" />
           </sus>
           <rel>
            <time value="0.086" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elvol>
         <elcut syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.486" pos="0" />
           </hold>
           <dec>
            <time value="0.486" pos="0" />
           </dec>
           <sus>
            <time value="0.486" pos="0" />
           </sus>
           <rel>
            <time value="0.086" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elcut>
         <elres syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.486" pos="0" />
           </hold>
           <dec>
            <time value="0.486" pos="0" />
           </dec>
           <sus>
            <time value="0.486" pos="0" />
           </sus>
           <rel>
            <time value="0.086" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elres>
        </eldata>
        <arpandchords arpdisabled="1" syncmode="0" chorddisabled="1" >
         <automation-pattern>
          <chord>
           <time value="0" pos="0" />
          </chord>
          <chordrange>
           <time value="1" pos="0" />
          </chordrange>
          <arp>
           <time value="0" pos="0" />
          </arp>
          <arprange>
           <time value="3" pos="0" />
          </arprange>
          <arptime>
           <time value="608" pos="0" />
          </arptime>
          <arptime_numerator>
           <time value="1" pos="0" />
          </arptime_numerator>
          <arptime_denominator>
           <time value="1" pos="0" />
          </arptime_denominator>
          <arpgate>
           <time value="192" pos="0" />
          </arpgate>
          <arpdir>
           <time value="2" pos="0" />
          </arpdir>
          <arpmode>
           <time value="0" pos="0" />
          </arpmode>
         </automation-pattern>
        </arpandchords>
        <midi>
         <automation-pattern>
          <inputchannel>
           <time value="0" pos="0" />
          </inputchannel>
          <outputchannel>
           <time value="1" pos="0" />
          </outputchannel>
          <receive>
           <time value="0" pos="0" />
          </receive>
          <send>
           <time value="0" pos="0" />
          </send>
          <defvelin>
           <time value="0" pos="0" />
          </defvelin>
          <defvelout>
           <time value="0" pos="0" />
          </defvelout>
         </automation-pattern>
        </midi>
        <fx fxdisabled="1" >
         <rack numofeffects="0" />
        </fx>
       </instrumenttrack>
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="0" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="64" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="128" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="192" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="256" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="20" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="36" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="48" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="320" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="384" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="448" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="172" pos="20" len="-64" />
        <note tone="9" pan="0" oct="4" vol="168" pos="24" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
        <note tone="9" pan="0" oct="4" vol="122" pos="40" len="-64" />
        <note tone="9" pan="0" oct="4" vol="144" pos="48" len="-64" />
        <note tone="9" pan="0" oct="4" vol="200" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="512" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="576" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="640" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="704" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="20" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
        <note tone="9" pan="0" oct="4" vol="98" pos="36" len="-64" />
        <note tone="9" pan="0" oct="4" vol="104" pos="40" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="48" len="-64" />
        <note tone="9" pan="0" oct="4" vol="102" pos="52" len="-64" />
        <note tone="9" pan="0" oct="4" vol="106" pos="56" len="-64" />
        <note tone="9" pan="0" oct="4" vol="104" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="768" frozen="0" len="64" />
      </track>
      <track muted="0" height="32" type="0" >
       <instrumenttrack width="250" x="253" y="199" height="436" name="kick_soft02.ogg" tab="2" visible="0" >
        <automation-pattern>
         <vol>
          <time value="90" pos="0" />
         </vol>
         <surpos-x>
          <time value="0" pos="0" />
         </surpos-x>
         <surpos-y>
          <time value="0" pos="0" />
         </surpos-y>
         <fxch>
          <time value="0" pos="0" />
         </fxch>
         <basenote>
          <time value="57" pos="0" />
         </basenote>
        </automation-pattern>
        <audiofileprocessor reversed="0" looped="0" eframe="0.999393" sframe="0" amp="200" src="drums/kick_soft02.ogg" />
        <eldata fwet="1" >
         <automation-pattern>
          <ftype>
           <time value="7" pos="0" />
          </ftype>
          <fcut>
           <time value="2720" pos="0" />
          </fcut>
          <fres>
           <time value="0.44" pos="0" />
          </fres>
         </automation-pattern>
         <elvol syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.99" pos="0" />
           </hold>
           <dec>
            <time value="0.49" pos="0" />
           </dec>
           <sus>
            <time value="0.839" pos="0" />
           </sus>
           <rel>
            <time value="0.696" pos="0" />
           </rel>
           <amt>
            <time value="1" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elvol>
         <elcut syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.49" pos="0" />
           </hold>
           <dec>
            <time value="0.49" pos="0" />
           </dec>
           <sus>
            <time value="0.49" pos="0" />
           </sus>
           <rel>
            <time value="0.99" pos="0" />
           </rel>
           <amt>
            <time value="1" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elcut>
         <elres syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.49" pos="0" />
           </hold>
           <dec>
            <time value="0.49" pos="0" />
           </dec>
           <sus>
            <time value="0.49" pos="0" />
           </sus>
           <rel>
            <time value="0.09" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elres>
        </eldata>
        <arpandchords arpdisabled="1" syncmode="0" chorddisabled="0" >
         <automation-pattern>
          <chord>
           <time value="0" pos="0" />
          </chord>
          <chordrange>
           <time value="2" pos="0" />
          </chordrange>
          <arp>
           <time value="0" pos="0" />
          </arp>
          <arprange>
           <time value="1" pos="0" />
          </arprange>
          <arptime>
           <time value="100" pos="0" />
          </arptime>
          <arptime_numerator>
           <time value="1" pos="0" />
          </arptime_numerator>
          <arptime_denominator>
           <time value="1" pos="0" />
          </arptime_denominator>
          <arpgate>
           <time value="100" pos="0" />
          </arpgate>
          <arpdir>
           <time value="0" pos="0" />
          </arpdir>
          <arpmode>
           <time value="0" pos="0" />
          </arpmode>
         </automation-pattern>
        </arpandchords>
        <midi>
         <automation-pattern>
          <inputchannel>
           <time value="0" pos="0" />
          </inputchannel>
          <outputchannel>
           <time value="1" pos="0" />
          </outputchannel>
          <receive>
           <time value="0" pos="0" />
          </receive>
          <send>
           <time value="0" pos="0" />
          </send>
          <defvelin>
           <time value="0" pos="0" />
          </defvelin>
          <defvelout>
           <time value="0" pos="0" />
          </defvelout>
         </automation-pattern>
        </midi>
        <fx fxdisabled="1" >
         <rack numofeffects="0" />
        </fx>
       </instrumenttrack>
       <pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="0" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="64" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="128" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="158" pos="4" len="-64" />
        <note tone="9" pan="0" oct="4" vol="58" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="20" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
        <note tone="9" pan="0" oct="4" vol="148" pos="32" len="-64" />
        <note tone="9" pan="0" oct="4" vol="154" pos="36" len="-64" />
        <note tone="9" pan="0" oct="4" vol="152" pos="40" len="-64" />
        <note tone="9" pan="0" oct="4" vol="186" pos="48" len="-64" />
        <note tone="9" pan="0" oct="4" vol="188" pos="52" len="-64" />
        <note tone="9" pan="0" oct="4" vol="188" pos="56" len="-64" />
        <note tone="9" pan="0" oct="4" vol="190" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="192" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="256" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="320" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="384" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="44" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="448" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="512" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="576" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="640" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="704" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="kick_soft02.ogg" pos="768" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="20" len="-64" />
        <note tone="9" pan="0" oct="4" vol="174" pos="24" len="-64" />
        <note tone="9" pan="0" oct="4" vol="170" pos="36" len="-64" />
        <note tone="9" pan="0" oct="4" vol="106" pos="40" len="-64" />
       </pattern>
      </track>
      <track muted="0" height="32" type="0" >
       <instrumenttrack width="250" x="0" y="199" height="436" name="snare03.ogg" tab="2" visible="0" >
        <automation-pattern>
         <vol>
          <time value="28" pos="0" />
         </vol>
         <surpos-x>
          <time value="512" pos="0" />
         </surpos-x>
         <surpos-y>
          <time value="-853" pos="0" />
         </surpos-y>
         <fxch>
          <time value="0" pos="0" />
         </fxch>
         <basenote>
          <time value="57" pos="0" />
         </basenote>
        </automation-pattern>
        <audiofileprocessor reversed="0" looped="0" eframe="0.999138" sframe="0" amp="100" src="drums/snare03.ogg" />
        <eldata fwet="1" >
         <automation-pattern>
          <ftype>
           <time value="7" pos="0" />
          </ftype>
          <fcut>
           <time value="800" pos="0" />
          </fcut>
          <fres>
           <time value="1.63" pos="0" />
          </fres>
         </automation-pattern>
         <elvol syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.49" pos="0" />
           </hold>
           <dec>
            <time value="0.49" pos="0" />
           </dec>
           <sus>
            <time value="0.968" pos="0" />
           </sus>
           <rel>
            <time value="0.816" pos="0" />
           </rel>
           <amt>
            <time value="1" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elvol>
         <elcut syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.49" pos="0" />
           </hold>
           <dec>
            <time value="0.49" pos="0" />
           </dec>
           <sus>
            <time value="0.49" pos="0" />
           </sus>
           <rel>
            <time value="0.09" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elcut>
         <elres syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.49" pos="0" />
           </hold>
           <dec>
            <time value="0.49" pos="0" />
           </dec>
           <sus>
            <time value="0.49" pos="0" />
           </sus>
           <rel>
            <time value="0.09" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elres>
        </eldata>
        <arpandchords arpdisabled="0" syncmode="0" chorddisabled="1" >
         <automation-pattern>
          <chord>
           <time value="0" pos="0" />
          </chord>
          <chordrange>
           <time value="3" pos="0" />
          </chordrange>
          <arp>
           <time value="0" pos="0" />
          </arp>
          <arprange>
           <time value="2" pos="0" />
          </arprange>
          <arptime>
           <time value="450" pos="0" />
          </arptime>
          <arptime_numerator>
           <time value="1" pos="0" />
          </arptime_numerator>
          <arptime_denominator>
           <time value="1" pos="0" />
          </arptime_denominator>
          <arpgate>
           <time value="200" pos="0" />
          </arpgate>
          <arpdir>
           <time value="2" pos="0" />
          </arpdir>
          <arpmode>
           <time value="0" pos="0" />
          </arpmode>
         </automation-pattern>
        </arpandchords>
        <midi>
         <automation-pattern>
          <inputchannel>
           <time value="0" pos="0" />
          </inputchannel>
          <outputchannel>
           <time value="1" pos="0" />
          </outputchannel>
          <receive>
           <time value="0" pos="0" />
          </receive>
          <send>
           <time value="0" pos="0" />
          </send>
          <defvelin>
           <time value="0" pos="0" />
          </defvelin>
          <defvelout>
           <time value="0" pos="0" />
          </defvelout>
         </automation-pattern>
        </midi>
        <fx fxdisabled="1" >
         <rack numofeffects="0" />
        </fx>
       </instrumenttrack>
       <pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="0" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="64" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="128" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="138" pos="4" len="-64" />
        <note tone="9" pan="0" oct="4" vol="52" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="176" pos="24" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="36" len="-64" />
        <note tone="9" pan="0" oct="4" vol="162" pos="40" len="-64" />
        <note tone="9" pan="0" oct="4" vol="158" pos="52" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
        <note tone="9" pan="0" oct="4" vol="180" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="192" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="256" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="320" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="384" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="36" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="448" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="512" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="576" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="640" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="704" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snare03.ogg" pos="768" frozen="0" len="64" />
      </track>
      <track muted="0" height="32" type="0" >
       <instrumenttrack width="250" x="513" y="199" height="436" name="wood01.ogg" tab="2" visible="0" >
        <automation-pattern>
         <vol>
          <time value="56" pos="0" />
         </vol>
         <surpos-x>
          <time value="0" pos="0" />
         </surpos-x>
         <surpos-y>
          <time value="0" pos="0" />
         </surpos-y>
         <fxch>
          <time value="0" pos="0" />
         </fxch>
         <basenote>
          <time value="48" pos="0" />
         </basenote>
        </automation-pattern>
        <audiofileprocessor reversed="0" looped="0" eframe="0.994132" sframe="0" amp="145" src="drums/wood01.ogg" />
        <eldata fwet="1" >
         <automation-pattern>
          <ftype>
           <time value="7" pos="0" />
          </ftype>
          <fcut>
           <time value="2080" pos="0" />
          </fcut>
          <fres>
           <time value="1.28" pos="0" />
          </fres>
         </automation-pattern>
         <elvol syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.49" pos="0" />
           </hold>
           <dec>
            <time value="0.49" pos="0" />
           </dec>
           <sus>
            <time value="0.49" pos="0" />
           </sus>
           <rel>
            <time value="0.09" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elvol>
         <elcut syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.49" pos="0" />
           </hold>
           <dec>
            <time value="0.49" pos="0" />
           </dec>
           <sus>
            <time value="0.49" pos="0" />
           </sus>
           <rel>
            <time value="0.09" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elcut>
         <elres syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.49" pos="0" />
           </hold>
           <dec>
            <time value="0.49" pos="0" />
           </dec>
           <sus>
            <time value="0.49" pos="0" />
           </sus>
           <rel>
            <time value="0.09" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elres>
        </eldata>
        <arpandchords arpdisabled="1" syncmode="0" chorddisabled="1" >
         <automation-pattern>
          <chord>
           <time value="0" pos="0" />
          </chord>
          <chordrange>
           <time value="1" pos="0" />
          </chordrange>
          <arp>
           <time value="0" pos="0" />
          </arp>
          <arprange>
           <time value="4" pos="0" />
          </arprange>
          <arptime>
           <time value="888" pos="0" />
          </arptime>
          <arptime_numerator>
           <time value="1" pos="0" />
          </arptime_numerator>
          <arptime_denominator>
           <time value="1" pos="0" />
          </arptime_denominator>
          <arpgate>
           <time value="200" pos="0" />
          </arpgate>
          <arpdir>
           <time value="0" pos="0" />
          </arpdir>
          <arpmode>
           <time value="0" pos="0" />
          </arpmode>
         </automation-pattern>
        </arpandchords>
        <midi>
         <automation-pattern>
          <inputchannel>
           <time value="0" pos="0" />
          </inputchannel>
          <outputchannel>
           <time value="1" pos="0" />
          </outputchannel>
          <receive>
           <time value="0" pos="0" />
          </receive>
          <send>
           <time value="0" pos="0" />
          </send>
          <defvelin>
           <time value="0" pos="0" />
          </defvelin>
          <defvelout>
           <time value="0" pos="0" />
          </defvelout>
         </automation-pattern>
        </midi>
        <fx fxdisabled="1" >
         <rack numofeffects="0" />
        </fx>
       </instrumenttrack>
       <pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="0" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="64" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="128" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="192" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="256" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="320" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="40" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="384" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="448" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="512" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="576" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
        <note tone="9" pan="0" oct="4" vol="58" pos="8" len="-64" />
        <note tone="9" pan="0" oct="4" vol="176" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="20" len="-64" />
        <note tone="9" pan="0" oct="4" vol="60" pos="24" len="-64" />
        <note tone="9" pan="0" oct="4" vol="170" pos="28" len="-64" />
        <note tone="9" pan="0" oct="4" vol="108" pos="40" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
        <note tone="9" pan="0" oct="4" vol="200" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="640" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="20" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="36" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="40" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="704" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="20" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="36" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="40" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="48" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="wood01.ogg" pos="768" frozen="0" len="64" />
      </track>
      <track muted="0" height="32" type="0" >
       <instrumenttrack width="250" x="260" y="0" height="436" name="snaph01.ogg" tab="1" visible="0" >
        <automation-pattern>
         <vol>
          <time value="200" pos="0" />
         </vol>
         <surpos-x>
          <time value="0" pos="0" />
         </surpos-x>
         <surpos-y>
          <time value="0" pos="0" />
         </surpos-y>
         <fxch>
          <time value="0" pos="0" />
         </fxch>
         <basenote>
          <time value="57" pos="0" />
         </basenote>
        </automation-pattern>
        <audiofileprocessor reversed="0" looped="0" eframe="0.996347" sframe="0" amp="120" src="misc/snaph01.ogg" />
        <eldata fwet="1" >
         <automation-pattern>
          <ftype>
           <time value="7" pos="0" />
          </ftype>
          <fcut>
           <time value="640" pos="0" />
          </fcut>
          <fres>
           <time value="10" pos="0" />
          </fres>
         </automation-pattern>
         <elvol syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.581" pos="0" />
           </hold>
           <dec>
            <time value="0.485" pos="0" />
           </dec>
           <sus>
            <time value="0.211" pos="0" />
           </sus>
           <rel>
            <time value="0.152" pos="0" />
           </rel>
           <amt>
            <time value="0.895" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0.162" pos="0" />
           </latt>
           <lspd>
            <time value="0.1384" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="1" pos="0" />
           </lamt>
           <x100>
            <time value="1" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elvol>
         <elcut syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0.077" pos="0" />
           </att>
           <hold>
            <time value="0.558" pos="0" />
           </hold>
           <dec>
            <time value="0.485" pos="0" />
           </dec>
           <sus>
            <time value="0.544" pos="0" />
           </sus>
           <rel>
            <time value="0.434" pos="0" />
           </rel>
           <amt>
            <time value="-0.295" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elcut>
         <elres syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.485" pos="0" />
           </hold>
           <dec>
            <time value="0.485" pos="0" />
           </dec>
           <sus>
            <time value="0.798" pos="0" />
           </sus>
           <rel>
            <time value="0.085" pos="0" />
           </rel>
           <amt>
            <time value="0.64" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elres>
        </eldata>
        <arpandchords arpdisabled="1" syncmode="0" chorddisabled="1" >
         <automation-pattern>
          <chord>
           <time value="0" pos="0" />
          </chord>
          <chordrange>
           <time value="4" pos="0" />
          </chordrange>
          <arp>
           <time value="0" pos="0" />
          </arp>
          <arprange>
           <time value="3" pos="0" />
          </arprange>
          <arptime>
           <time value="608" pos="0" />
          </arptime>
          <arptime_numerator>
           <time value="1" pos="0" />
          </arptime_numerator>
          <arptime_denominator>
           <time value="1" pos="0" />
          </arptime_denominator>
          <arpgate>
           <time value="192" pos="0" />
          </arpgate>
          <arpdir>
           <time value="2" pos="0" />
          </arpdir>
          <arpmode>
           <time value="0" pos="0" />
          </arpmode>
         </automation-pattern>
        </arpandchords>
        <midi>
         <automation-pattern>
          <inputchannel>
           <time value="0" pos="0" />
          </inputchannel>
          <outputchannel>
           <time value="1" pos="0" />
          </outputchannel>
          <receive>
           <time value="0" pos="0" />
          </receive>
          <send>
           <time value="0" pos="0" />
          </send>
          <defvelin>
           <time value="0" pos="0" />
          </defvelin>
          <defvelout>
           <time value="0" pos="0" />
          </defvelout>
         </automation-pattern>
        </midi>
        <fx fxdisabled="1" >
         <rack numofeffects="0" />
        </fx>
       </instrumenttrack>
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="0" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="64" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="128" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="192" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="256" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="320" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="384" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="448" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="512" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="40" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="576" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="640" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="704" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="snaph01.ogg" pos="768" frozen="0" len="64" />
      </track>
      <track muted="0" height="32" type="0" >
       <instrumenttrack width="250" x="514" y="0" height="436" name="tom05.ogg" tab="1" visible="0" >
        <automation-pattern>
         <vol>
          <time value="100" pos="0" />
         </vol>
         <surpos-x>
          <time value="0" pos="0" />
         </surpos-x>
         <surpos-y>
          <time value="0" pos="0" />
         </surpos-y>
         <fxch>
          <time value="0" pos="0" />
         </fxch>
         <basenote>
          <time value="57" pos="0" />
         </basenote>
        </automation-pattern>
        <audiofileprocessor reversed="0" looped="0" eframe="0.999672" sframe="0" amp="100" src="drums/tom05.ogg" />
        <eldata fwet="1" >
         <automation-pattern>
          <ftype>
           <time value="7" pos="0" />
          </ftype>
          <fcut>
           <time value="160" pos="0" />
          </fcut>
          <fres>
           <time value="2.81" pos="0" />
          </fres>
         </automation-pattern>
         <elvol syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.495" pos="0" />
           </hold>
           <dec>
            <time value="0.495" pos="0" />
           </dec>
           <sus>
            <time value="0.495" pos="0" />
           </sus>
           <rel>
            <time value="0.095" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elvol>
         <elcut syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0" pos="0" />
           </att>
           <hold>
            <time value="0.495" pos="0" />
           </hold>
           <dec>
            <time value="0.495" pos="0" />
           </dec>
           <sus>
            <time value="0.495" pos="0" />
           </sus>
           <rel>
            <time value="0.095" pos="0" />
           </rel>
           <amt>
            <time value="0" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elcut>
         <elres syncmode="0" userwavefile="" >
          <automation-pattern>
           <pdel>
            <time value="0" pos="0" />
           </pdel>
           <att>
            <time value="0.128" pos="0" />
           </att>
           <hold>
            <time value="0.687" pos="0" />
           </hold>
           <dec>
            <time value="0.495" pos="0" />
           </dec>
           <sus>
            <time value="0.683" pos="0" />
           </sus>
           <rel>
            <time value="0.095" pos="0" />
           </rel>
           <amt>
            <time value="0.51" pos="0" />
           </amt>
           <lshp>
            <time value="0" pos="0" />
           </lshp>
           <lpdel>
            <time value="0" pos="0" />
           </lpdel>
           <latt>
            <time value="0" pos="0" />
           </latt>
           <lspd>
            <time value="0.1" pos="0" />
           </lspd>
           <lspd_numerator>
            <time value="1" pos="0" />
           </lspd_numerator>
           <lspd_denominator>
            <time value="1" pos="0" />
           </lspd_denominator>
           <lamt>
            <time value="0.01" pos="0" />
           </lamt>
           <x100>
            <time value="0" pos="0" />
           </x100>
           <ctlenvamt>
            <time value="0" pos="0" />
           </ctlenvamt>
          </automation-pattern>
         </elres>
        </eldata>
        <arpandchords arpdisabled="1" syncmode="0" chorddisabled="1" >
         <automation-pattern>
          <chord>
           <time value="0" pos="0" />
          </chord>
          <chordrange>
           <time value="1" pos="0" />
          </chordrange>
          <arp>
           <time value="0" pos="0" />
          </arp>
          <arprange>
           <time value="1" pos="0" />
          </arprange>
          <arptime>
           <time value="100" pos="0" />
          </arptime>
          <arptime_numerator>
           <time value="1" pos="0" />
          </arptime_numerator>
          <arptime_denominator>
           <time value="1" pos="0" />
          </arptime_denominator>
          <arpgate>
           <time value="100" pos="0" />
          </arpgate>
          <arpdir>
           <time value="0" pos="0" />
          </arpdir>
          <arpmode>
           <time value="0" pos="0" />
          </arpmode>
         </automation-pattern>
        </arpandchords>
        <midi>
         <automation-pattern>
          <inputchannel>
           <time value="0" pos="0" />
          </inputchannel>
          <outputchannel>
           <time value="1" pos="0" />
          </outputchannel>
          <receive>
           <time value="0" pos="0" />
          </receive>
          <send>
           <time value="0" pos="0" />
          </send>
          <defvelin>
           <time value="0" pos="0" />
          </defvelin>
          <defvelout>
           <time value="0" pos="0" />
          </defvelout>
         </automation-pattern>
        </midi>
        <fx fxdisabled="1" >
         <rack numofeffects="0" />
        </fx>
       </instrumenttrack>
       <pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="0" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="64" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="128" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="192" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="256" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="320" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="384" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="448" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="512" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="576" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="640" frozen="0" len="64" >
        <note tone="9" pan="0" oct="4" vol="100" pos="4" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="28" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="36" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="40" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="52" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
        <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
       </pattern>
       <pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="704" frozen="0" len="64" />
       <pattern steps="16" muted="0" type="0" name="tom05.ogg" pos="768" frozen="0" len="64" />
      </track>
     </trackcontainer>
    </bbtrack>
    <bbtco muted="0" name="start" color="4282417407" pos="256" len="64" />
    <bbtco muted="0" name="start" color="4282417407" pos="4352" len="64" />
    <bbtco muted="0" name="start" color="4282417407" pos="6144" len="64" />
    <bbtco muted="0" name="start" color="4282417407" pos="2304" len="64" />
    <bbtco muted="0" name="start" color="4282417407" pos="8448" len="64" />
   </track>
   <track muted="0" height="32" type="1" >
    <bbtrack icon="" name="hrrrrrrrrrr" />
    <bbtco muted="0" name="hrrrrrrrrrr" color="4282417407" pos="0" len="768" />
    <bbtco muted="0" name="hrrrrrrrrrr" color="4282417407" pos="2048" len="764" />
    <bbtco muted="0" name="hrrrrrrrrrr" color="4282417407" pos="5888" len="2048" />
    <bbtco muted="0" name="hrrrrrrrrrr" color="4282417407" pos="4096" len="764" />
    <bbtco muted="0" name="hrrrrrrrrrr" color="4282417407" pos="8192" len="260" />
   </track>
   <track muted="0" height="32" type="1" >
    <bbtrack icon="" name="trrrrrrrrrrrrr" />
    <bbtco muted="0" name="trrrrrrrrrrrrr" color="4282417407" pos="2240" len="192" />
    <bbtco muted="0" name="trrrrrrrrrrrrr" color="4282417407" pos="6144" len="64" />
   </track>
   <track muted="0" height="32" type="1" >
    <bbtrack icon="" name="beat1" />
    <bbtco muted="0" name="beat1" color="4282417407" pos="256" len="2044" />
    <bbtco muted="0" name="beat1" color="4282417407" pos="4352" len="4092" />
   </track>
   <track muted="0" height="32" type="1" >
    <bbtrack icon="" name="first lap snap" />
    <bbtco muted="0" name="first lap snap" color="4282417407" pos="252" len="1024" />
    <bbtco muted="0" name="first lap snap" color="4282417407" pos="4612" len="248" />
    <bbtco muted="0" name="first lap snap" color="4282417407" pos="5120" len="256" />
    <bbtco muted="0" name="first lap snap" color="4282417407" pos="5632" len="252" />
    <bbtco muted="0" name="first lap snap" color="4282417407" pos="7680" len="256" />
   </track>
   <track muted="0" height="32" type="1" >
    <bbtrack icon="" name="fist lap wood" />
    <bbtco muted="0" name="fist lap wood" color="4282417407" pos="1280" len="1020" />
    <bbtco muted="0" name="fist lap wood" color="4282417407" pos="7424" len="256" />
   </track>
   <track muted="0" height="32" type="1" >
    <bbtrack icon="" name="beat2" />
    <bbtco muted="0" name="beat2" color="4282417407" pos="2304" len="2048" />
   </track>
   <track muted="0" height="32" type="1" >
    <bbtrack icon="" name="second lap snap" />
    <bbtco muted="0" name="first lap snap" color="4282417407" pos="2304" len="1024" />
    <bbtco muted="0" name="second lap snap" color="4282417407" pos="4864" len="252" />
    <bbtco muted="0" name="second lap snap" color="4282417407" pos="5632" len="512" />
    <bbtco muted="0" name="second lap snap" color="4282417407" pos="7168" len="256" />
   </track>
   <track muted="0" height="32" type="1" >
    <bbtrack icon="" name="third lap snap" />
    <bbtco muted="0" name="third lap snap" color="4282417407" pos="4352" len="1016" />
    <bbtco muted="0" name="third lap snap" color="4282417407" pos="6656" len="256" />
   </track>
   <track muted="0" height="32" type="1" >
    <bbtrack icon="" name="second lap wood" />
    <bbtco muted="0" name="fist lap wood" color="4282417407" pos="3328" len="1024" />
    <bbtco muted="0" name="second lap wood" color="4282417407" pos="6912" len="256" />
   </track>
   <track muted="0" height="32" type="1" >
    <bbtrack icon="" name="third lap wood" />
    <bbtco muted="0" name="third lap wood" color="4282417407" pos="5120" len="1536" />
   </track>
   <track muted="0" height="32" type="1" >
    <bbtrack icon="" name="final" />
    <bbtco muted="0" name="final" color="4282417407" pos="7932" len="512" />
   </track>
   <track muted="0" height="32" type="1" >
    <bbtrack icon="" name="final beat" />
    <bbtco muted="0" name="final beat" color="4282417407" pos="6144" len="2048" />
   </track>
  </trackcontainer>
  <pianoroll width="640" x="0" y="0" height="480" visible="0" />
  <automation-editor width="640" x="0" y="0" height="480" visible="0" />
  <projectnotes width="300" x="0" y="197" height="200" visible="1" ><![CDATA[<html><head><meta name="qrichtext" content="1" /></head><body style="font-size:10pt;font-family:Sans Serif">
<p>license:GPL version2</p>
<p>A race betwin instruments. :)</p>
<p>(c)  zvonsully@gmail.com 2006 </p>
</body></html>
]]></projectnotes>
  <timeline lp1pos="64" lp0pos="0" lpstate="0" />
 </song>
</multimediaproject>
