<?xml version="1.0"?>
<!DOCTYPE multimedia-project>
<multimediaproject creator="Linux MultiMedia Studio (LMMS)" creatorversion="0.2.1" type="song" version="1.0" >
  <head>
    <automation-pattern>
      <bpm>
        <time value="170" pos="0" />
      </bpm>
      <mastervol>
        <time value="75" pos="0" />
      </mastervol>
      <masterpitch>
        <time value="0" pos="0" />
      </masterpitch>
    </automation-pattern>
  </head>
  <song>
    <trackcontainer width="580" x="0" y="0" height="300" type="songeditor" visible="1" >
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Base" >
          <trackcontainer width="504" x="0" y="0" height="300" type="bbeditor" visible="0" >
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="0" y="0" height="436" name="strings01.ogg" tab="1" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="48" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="-524" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="24" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999985" sframe="0" amp="100" src="stringsnpads/strings01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="1" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.51" pos="0" />
                      </dec>
                      <sus>
                        <time value="0" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.49" pos="0" />
                      </rel>
                      <amt>
                        <time value="1" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="1" name="strings01.ogg" pos="0" frozen="0" len="256" >
                <note tone="9" pan="0" oct="3" vol="100" pos="0" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="3" vol="100" pos="64" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="5" pan="0" oct="3" vol="100" pos="128" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="3" vol="100" pos="192" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="0" name="strings01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="strings01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="strings01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="strings01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="strings01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="strings01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="strings01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="strings01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="strings01.ogg" pos="576" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="0" y="0" height="436" name="space_strings01.ogg" tab="1" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="124" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="24" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.99998" sframe="0" amp="100" src="stringsnpads/space_strings01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.34" pos="0" />
                      </hold>
                      <dec>
                        <time value="1" pos="0" />
                      </dec>
                      <sus>
                        <time value="1" pos="0" />
                      </sus>
                      <rel>
                        <time value="1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0.96" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="space_strings01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="space_strings01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="space_strings01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="space_strings01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="space_strings01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="space_strings01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="space_strings01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="space_strings01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="1" name="space_strings01.ogg" pos="512" frozen="0" len="448" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="4" vol="100" pos="128" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="5" pan="0" oct="4" vol="100" pos="256" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="4" vol="100" pos="384" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="0" name="space_strings01.ogg" pos="576" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="0" y="0" height="436" name="nord_ambient01.ogg" tab="1" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="-474" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="24" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999985" sframe="0" amp="100" src="stringsnpads/nord_ambient01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="1" pos="0" />
                      </hold>
                      <dec>
                        <time value="1" pos="0" />
                      </dec>
                      <sus>
                        <time value="0" pos="0" />
                      </sus>
                      <rel>
                        <time value="1" pos="0" />
                      </rel>
                      <amt>
                        <time value="1" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="nord_ambient01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="nord_ambient01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="nord_ambient01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="nord_ambient01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="nord_ambient01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="nord_ambient01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="nord_ambient01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="nord_ambient01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="1" name="nord_ambient01.ogg" pos="512" frozen="0" len="512" >
                <note tone="9" pan="0" oct="4" vol="100" pos="64" len="128" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="192" len="128" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="320" len="128" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="448" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="0" name="nord_ambient01.ogg" pos="576" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="512" x="0" y="0" height="436" name="jungle01.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999976" sframe="0" amp="100" src="beats/jungle01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="jungle01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="jungle01.ogg" pos="64" frozen="0" len="64" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="-64" />
              </pattern>
              <pattern steps="16" muted="0" type="0" name="jungle01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="jungle01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="jungle01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="jungle01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="jungle01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="jungle01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="jungle01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="jungle01.ogg" pos="576" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="0" y="0" height="436" name="bassdrum03.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999701" sframe="0" amp="100" src="drums/bassdrum03.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="bassdrum03.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum03.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum03.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum03.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum03.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum03.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum03.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum03.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum03.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="64" muted="0" type="0" name="bassdrum03.ogg" pos="576" frozen="0" len="256" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="96" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="128" len="-64" />
              </pattern>
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="0" y="0" height="436" name="clap02.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="-174" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="424" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999568" sframe="0" amp="100" src="drums/clap02.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="clap02.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap02.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap02.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap02.ogg" pos="192" frozen="0" len="64" >
                <note tone="9" pan="0" oct="4" vol="100" pos="16" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="48" len="-64" />
              </pattern>
              <pattern steps="16" muted="0" type="0" name="clap02.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap02.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap02.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap02.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap02.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap02.ogg" pos="576" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="0" y="0" height="436" name="clap03.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="324" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="-24" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.99926" sframe="0" amp="100" src="drums/clap03.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="clap03.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap03.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap03.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap03.ogg" pos="192" frozen="0" len="64" >
                <note tone="9" pan="0" oct="4" vol="100" pos="8" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="40" len="-64" />
              </pattern>
              <pattern steps="16" muted="0" type="0" name="clap03.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap03.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap03.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap03.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap03.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="64" muted="0" type="0" name="clap03.ogg" pos="576" frozen="0" len="256" >
                <note tone="9" pan="0" oct="4" vol="100" pos="16" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="48" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="80" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="112" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="144" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="176" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="208" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="240" len="-64" />
              </pattern>
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="512" x="0" y="0" height="436" name="matrix1000_pluck01.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.99991" sframe="0" amp="100" src="basses/matrix1000_pluck01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="matrix1000_pluck01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="matrix1000_pluck01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="matrix1000_pluck01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="matrix1000_pluck01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="matrix1000_pluck01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="1" name="matrix1000_pluck01.ogg" pos="320" frozen="0" len="256" >
                <note tone="9" pan="0" oct="4" vol="100" pos="8" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="24" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="40" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="56" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="4" vol="100" pos="72" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="4" vol="100" pos="88" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="4" vol="100" pos="104" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="4" vol="100" pos="120" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="5" pan="0" oct="4" vol="100" pos="136" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="5" pan="0" oct="4" vol="100" pos="152" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="5" pan="0" oct="4" vol="100" pos="168" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="5" pan="0" oct="4" vol="100" pos="184" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="4" vol="100" pos="200" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="4" vol="100" pos="216" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="4" vol="100" pos="232" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="4" vol="100" pos="248" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="0" name="matrix1000_pluck01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="matrix1000_pluck01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="matrix1000_pluck01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="matrix1000_pluck01.ogg" pos="576" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="512" x="0" y="0" height="436" name="kick_distorted01.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999821" sframe="0" amp="100" src="drums/kick_distorted01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="128" frozen="0" len="64" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="16" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="48" len="-64" />
              </pattern>
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="192" frozen="0" len="64" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="16" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="48" len="-64" />
              </pattern>
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="576" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="0" y="0" height="436" name="shaker03.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="48" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="374" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="-24" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.998949" sframe="0" amp="100" src="drums/shaker03.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="shaker03.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="shaker03.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="shaker03.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="shaker03.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="shaker03.ogg" pos="256" frozen="0" len="64" >
                <note tone="9" pan="0" oct="4" vol="100" pos="8" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="12" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="24" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="28" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="40" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="44" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="56" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="60" len="-64" />
              </pattern>
              <pattern steps="16" muted="0" type="0" name="shaker03.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="shaker03.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="shaker03.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="shaker03.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="shaker03.ogg" pos="576" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="0" y="0" height="436" name="piano02.ogg" tab="1" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="62" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="-374" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="24" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999991" sframe="0" amp="100" src="instruments/piano02.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.98" pos="0" />
                      </rel>
                      <amt>
                        <time value="1" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="1" name="piano02.ogg" pos="384" frozen="0" len="1024" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="16" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="32" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="48" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="5" vol="100" pos="56" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="64" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="80" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="96" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="112" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="5" pan="0" oct="5" vol="100" pos="128" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="5" pan="0" oct="5" vol="100" pos="144" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="5" pan="0" oct="5" vol="100" pos="160" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="5" pan="0" oct="5" vol="100" pos="176" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="10" pan="0" oct="5" vol="100" pos="184" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="192" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="208" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="224" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="240" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="6" vol="100" pos="256" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="6" vol="100" pos="272" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="6" vol="100" pos="288" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="6" vol="100" pos="304" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="10" pan="0" oct="5" vol="100" pos="312" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="320" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="336" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="352" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="368" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="5" vol="100" pos="384" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="5" vol="100" pos="400" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="5" vol="100" pos="416" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="5" vol="100" pos="432" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="10" pan="0" oct="5" vol="100" pos="440" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="448" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="464" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="480" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="496" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="512" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="528" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="544" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="560" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="5" vol="100" pos="568" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="576" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="592" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="608" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="624" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="640" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="656" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="672" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="688" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="5" vol="100" pos="696" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="704" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="720" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="736" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="752" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="6" vol="100" pos="768" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="6" vol="100" pos="784" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="6" vol="100" pos="800" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="6" vol="100" pos="816" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="10" pan="0" oct="5" vol="100" pos="824" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="832" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="848" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="864" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="5" vol="100" pos="880" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="5" vol="100" pos="896" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="5" vol="100" pos="912" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="5" vol="100" pos="928" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="5" vol="100" pos="944" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="3" pan="0" oct="5" vol="100" pos="952" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="960" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="976" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="992" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="1008" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="576" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="512" x="0" y="0" height="436" name="violin_pizzicato01.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.99978" sframe="0" amp="100" src="instruments/violin_pizzicato01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="violin_pizzicato01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="violin_pizzicato01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="violin_pizzicato01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="violin_pizzicato01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="violin_pizzicato01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="violin_pizzicato01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="violin_pizzicato01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="violin_pizzicato01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="violin_pizzicato01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="violin_pizzicato01.ogg" pos="576" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="0" y="0" height="436" name="harpsichord01.ogg" tab="1" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="56" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="324" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="-24" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999977" sframe="0" amp="100" src="instruments/harpsichord01.ogg" />
                <eldata fwet="1" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="1" pos="0" />
                      </rel>
                      <amt>
                        <time value="1" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="1" name="harpsichord01.ogg" pos="448" frozen="0" len="1024" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="4" vol="100" pos="24" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="32" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="10" pan="0" oct="4" vol="100" pos="56" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="64" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="128" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="5" vol="100" pos="152" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="10" pan="0" oct="4" vol="100" pos="160" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="5" vol="100" pos="184" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="192" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="256" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="4" vol="100" pos="280" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="288" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="10" pan="0" oct="4" vol="100" pos="312" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="320" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="10" pan="0" oct="4" vol="100" pos="384" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="5" vol="100" pos="408" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="416" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="5" vol="100" pos="440" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="448" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="512" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="4" vol="100" pos="536" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="544" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="10" pan="0" oct="4" vol="100" pos="568" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="576" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="4" vol="100" pos="640" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="664" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="10" pan="0" oct="4" vol="100" pos="672" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="5" vol="100" pos="696" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="704" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="768" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="4" vol="100" pos="792" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="800" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="10" pan="0" oct="4" vol="100" pos="824" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="832" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="5" vol="100" pos="896" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="920" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="0" pan="0" oct="5" vol="100" pos="928" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="10" pan="0" oct="4" vol="100" pos="952" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="960" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="576" frozen="0" len="64" />
            </track>
          </trackcontainer>
        </bbtrack>
        <bbtco muted="0" name="Base" color="4282417407" pos="3072" len="1024" />
        <bbtco muted="0" name="Base" color="4282417407" pos="4096" len="1024" />
        <bbtco muted="0" name="Base" color="4282417407" pos="15360" len="1024" />
        <bbtco muted="0" name="Base" color="4282417407" pos="16384" len="1024" />
        <bbtco muted="0" name="Base" color="4282417407" pos="17408" len="1024" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Jungle" />
        <bbtco muted="0" name="Jungle" color="4282417407" pos="4096" len="1024" />
        <bbtco muted="0" name="Jungle" color="4282417407" pos="5120" len="1024" />
        <bbtco muted="0" name="Jungle" color="4282417407" pos="6144" len="1024" />
        <bbtco muted="0" name="Jungle" color="4282417407" pos="7168" len="1024" />
        <bbtco muted="0" name="Jungle" color="4282417407" pos="8192" len="1024" />
        <bbtco muted="0" name="Jungle" color="4282417407" pos="9728" len="448" />
        <bbtco muted="0" name="Jungle" color="4282417407" pos="10240" len="1024" />
        <bbtco muted="0" name="Jungle" color="4282417407" pos="11776" len="512" />
        <bbtco muted="0" name="Jungle" color="4282417407" pos="12288" len="1024" />
        <bbtco muted="0" name="Jungle" color="4282417407" pos="13312" len="1024" />
        <bbtco muted="0" name="Jungle" color="4282417407" pos="14336" len="1024" />
        <bbtco muted="0" name="Jungle" color="4282417407" pos="15360" len="1024" />
        <bbtco muted="0" name="Jungle" color="4282417407" pos="16384" len="1024" />
        <bbtco muted="0" name="Jungle" color="4282417407" pos="17408" len="768" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Beat" />
        <bbtco muted="0" name="Beat" color="4282417407" pos="1024" len="512" />
        <bbtco muted="0" name="Beat" color="4282417407" pos="2560" len="256" />
        <bbtco muted="0" name="Beat" color="4282417407" pos="2816" len="256" />
        <bbtco muted="0" name="Beat" color="4282417407" pos="3072" len="768" />
        <bbtco muted="0" name="Beat" color="4282417407" pos="4096" len="512" />
        <bbtco muted="0" name="Beat" color="4282417407" pos="6656" len="512" />
        <bbtco muted="0" name="Beat" color="4282417407" pos="7232" len="960" />
        <bbtco muted="0" name="Beat" color="4282417407" pos="15360" len="1024" />
        <bbtco muted="0" name="Beat" color="4282417407" pos="16448" len="960" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Beat2" />
        <bbtco muted="0" name="Beat2" color="4282417407" pos="1536" len="512" />
        <bbtco muted="0" name="Beat2" color="4282417407" pos="4608" len="512" />
        <bbtco muted="0" name="Beat2" color="4282417407" pos="5120" len="768" />
        <bbtco muted="0" name="Beat2" color="4282417407" pos="8192" len="1024" />
        <bbtco muted="0" name="Beat2" color="4282417407" pos="10240" len="1024" />
        <bbtco muted="0" name="Beat2" color="4282417407" pos="11264" len="1024" />
        <bbtco muted="0" name="Beat2" color="4282417407" pos="12416" len="896" />
        <bbtco muted="0" name="Beat2" color="4282417407" pos="13312" len="1024" />
        <bbtco muted="0" name="Beat2" color="4282417407" pos="14336" len="1024" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Shaker" />
        <bbtco muted="0" name="Shaker" color="4282417407" pos="5120" len="1024" />
        <bbtco muted="0" name="Shaker" color="4282417407" pos="7168" len="1024" />
        <bbtco muted="0" name="Shaker" color="4282417407" pos="8192" len="1024" />
        <bbtco muted="0" name="Shaker" color="4282417407" pos="10240" len="1024" />
        <bbtco muted="0" name="Shaker" color="4282417407" pos="11264" len="1024" />
        <bbtco muted="0" name="Shaker" color="4282417407" pos="13312" len="1024" />
        <bbtco muted="0" name="Shaker" color="4282417407" pos="17920" len="512" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Matrix" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="2048" len="256" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="2304" len="256" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="2560" len="256" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="2816" len="256" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="3072" len="1024" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="4096" len="1024" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="5120" len="1024" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="6144" len="1024" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="7168" len="1024" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="8192" len="1024" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="10240" len="1024" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="11264" len="1024" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="12288" len="1024" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="13312" len="1024" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="14336" len="1024" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="15360" len="1024" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="16384" len="1024" />
        <bbtco muted="0" name="Matrix" color="4282417407" pos="17408" len="1024" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Piano" />
        <bbtco muted="0" name="Piano" color="4282417407" pos="6144" len="1024" />
        <bbtco muted="0" name="Piano" color="4282417407" pos="7168" len="1024" />
        <bbtco muted="0" name="Piano" color="4282417407" pos="8192" len="1024" />
        <bbtco muted="0" name="Piano" color="4282417407" pos="9216" len="1024" />
        <bbtco muted="0" name="Piano" color="4282417407" pos="10240" len="1024" />
        <bbtco muted="0" name="Piano" color="4282417407" pos="12288" len="1024" />
        <bbtco muted="0" name="Piano" color="4282417407" pos="13312" len="1024" />
        <bbtco muted="0" name="Piano" color="4282417407" pos="14336" len="1024" />
        <bbtco muted="0" name="Piano" color="4282417407" pos="15360" len="1024" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Harp" />
        <bbtco muted="0" name="Harp" color="4282417407" pos="9216" len="1024" />
        <bbtco muted="0" name="Harp" color="4282417407" pos="10240" len="1024" />
        <bbtco muted="0" name="Harp" color="4282417407" pos="11264" len="1024" />
        <bbtco muted="0" name="Harp" color="4282417407" pos="12288" len="1024" />
        <bbtco muted="0" name="Harp" color="4282417407" pos="13312" len="1024" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Sounds" />
        <bbtco muted="0" name="Sounds" color="4282417407" pos="0" len="512" />
        <bbtco muted="0" name="Sounds" color="4282417407" pos="512" len="512" />
        <bbtco muted="0" name="Sounds" color="4282417407" pos="1024" len="512" />
        <bbtco muted="0" name="Sounds" color="4282417407" pos="1536" len="512" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Beat/Baseline 9" />
        <bbtco muted="0" name="Beat/Baseline 9" color="4282417407" pos="512" len="512" />
        <bbtco muted="0" name="Beat/Baseline 9" color="4282417407" pos="1024" len="512" />
      </track>
      <track muted="0" height="32" type="0" >
        <instrumenttrack width="250" x="0" y="0" height="436" name="space_strings01.ogg" tab="1" visible="0" >
          <automation-pattern>
            <vol>
              <time value="60" pos="0" />
            </vol>
            <surpos-x>
              <time value="574" pos="0" />
            </surpos-x>
            <surpos-y>
              <time value="-74" pos="0" />
            </surpos-y>
            <fxch>
              <time value="0" pos="0" />
            </fxch>
            <basenote>
              <time value="57" pos="0" />
            </basenote>
          </automation-pattern>
          <audiofileprocessor reversed="0" looped="0" eframe="0.999988" sframe="0" amp="100" src="stringsnpads/space_strings01.ogg" />
          <eldata fwet="0" >
            <automation-pattern>
              <ftype>
                <time value="0" pos="0" />
              </ftype>
              <fcut>
                <time value="14000" pos="0" />
              </fcut>
              <fres>
                <time value="0.5" pos="0" />
              </fres>
            </automation-pattern>
            <elvol lfosyncmode="0" userwavefile="" >
              <automation-pattern>
                <pdel>
                  <time value="0" pos="0" />
                </pdel>
                <att>
                  <time value="0" pos="0" />
                </att>
                <hold>
                  <time value="0.38" pos="0" />
                </hold>
                <dec>
                  <time value="1" pos="0" />
                </dec>
                <sus>
                  <time value="1" pos="0" />
                </sus>
                <rel>
                  <time value="0.1" pos="0" />
                </rel>
                <amt>
                  <time value="1" pos="0" />
                </amt>
                <lshp>
                  <time value="0" pos="0" />
                </lshp>
                <lpdel>
                  <time value="0" pos="0" />
                </lpdel>
                <latt>
                  <time value="0" pos="0" />
                </latt>
                <lspd>
                  <time value="0.1" pos="0" />
                </lspd>
                <lamt>
                  <time value="0" pos="0" />
                </lamt>
                <x100>
                  <time value="0" pos="0" />
                </x100>
                <ctlenvamt>
                  <time value="0" pos="0" />
                </ctlenvamt>
              </automation-pattern>
            </elvol>
            <elcut lfosyncmode="0" userwavefile="" >
              <automation-pattern>
                <pdel>
                  <time value="0" pos="0" />
                </pdel>
                <att>
                  <time value="0" pos="0" />
                </att>
                <hold>
                  <time value="0.5" pos="0" />
                </hold>
                <dec>
                  <time value="0.5" pos="0" />
                </dec>
                <sus>
                  <time value="0.5" pos="0" />
                </sus>
                <rel>
                  <time value="0.1" pos="0" />
                </rel>
                <amt>
                  <time value="0" pos="0" />
                </amt>
                <lshp>
                  <time value="0" pos="0" />
                </lshp>
                <lpdel>
                  <time value="0" pos="0" />
                </lpdel>
                <latt>
                  <time value="0" pos="0" />
                </latt>
                <lspd>
                  <time value="0.1" pos="0" />
                </lspd>
                <lamt>
                  <time value="0" pos="0" />
                </lamt>
                <x100>
                  <time value="0" pos="0" />
                </x100>
                <ctlenvamt>
                  <time value="0" pos="0" />
                </ctlenvamt>
              </automation-pattern>
            </elcut>
            <elres lfosyncmode="0" userwavefile="" >
              <automation-pattern>
                <pdel>
                  <time value="0" pos="0" />
                </pdel>
                <att>
                  <time value="0" pos="0" />
                </att>
                <hold>
                  <time value="0.5" pos="0" />
                </hold>
                <dec>
                  <time value="0.5" pos="0" />
                </dec>
                <sus>
                  <time value="0.5" pos="0" />
                </sus>
                <rel>
                  <time value="0.1" pos="0" />
                </rel>
                <amt>
                  <time value="0" pos="0" />
                </amt>
                <lshp>
                  <time value="0" pos="0" />
                </lshp>
                <lpdel>
                  <time value="0" pos="0" />
                </lpdel>
                <latt>
                  <time value="0" pos="0" />
                </latt>
                <lspd>
                  <time value="0.1" pos="0" />
                </lspd>
                <lamt>
                  <time value="0" pos="0" />
                </lamt>
                <x100>
                  <time value="0" pos="0" />
                </x100>
                <ctlenvamt>
                  <time value="0" pos="0" />
                </ctlenvamt>
              </automation-pattern>
            </elres>
          </eldata>
          <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
            <automation-pattern>
              <chord>
                <time value="0" pos="0" />
              </chord>
              <chordrange>
                <time value="1" pos="0" />
              </chordrange>
              <arp>
                <time value="0" pos="0" />
              </arp>
              <arprange>
                <time value="1" pos="0" />
              </arprange>
              <arptime>
                <time value="100" pos="0" />
              </arptime>
              <arpgate>
                <time value="100" pos="0" />
              </arpgate>
              <arpdir>
                <time value="0" pos="0" />
              </arpdir>
              <arpmode>
                <time value="0" pos="0" />
              </arpmode>
            </automation-pattern>
          </arpandchords>
          <midi>
            <automation-pattern>
              <inputchannel>
                <time value="0" pos="0" />
              </inputchannel>
              <outputchannel>
                <time value="1" pos="0" />
              </outputchannel>
              <receive>
                <time value="0" pos="0" />
              </receive>
              <send>
                <time value="0" pos="0" />
              </send>
              <defvelin>
                <time value="0" pos="0" />
              </defvelin>
              <defvelout>
                <time value="0" pos="0" />
              </defvelout>
            </automation-pattern>
          </midi>
        </instrumenttrack>
        <pattern steps="16" muted="0" type="1" name="space_strings01.ogg" pos="6080" frozen="0" len="64" >
          <note tone="9" pan="0" oct="4" vol="100" pos="0" len="64" >
            <automation-pattern>
              <detuning>
                <time value="0" pos="0" />
              </detuning>
            </automation-pattern>
          </note>
        </pattern>
      </track>
    </trackcontainer>
    <pianoroll width="640" x="0" y="0" height="480" visible="0" />
    <automation-editor width="640" x="0" y="0" height="480" visible="0" />
    <projectnotes width="300" x="0" y="0" height="200" visible="0" ><![CDATA[<html><head><meta name="qrichtext" content="1" /></head><body style="font-size:9pt;font-family:DejaVu Sans">
<p>Put down your project notes here.</p>
</body></html>
]]></projectnotes>
    <timeline lp1pos="1024" lp0pos="512" lpstate="0" />
  </song>
</multimediaproject>
