<?xml version="1.0"?>
<!DOCTYPE multimedia-project>
<multimediaproject creator="Linux MultiMedia Studio (LMMS)" creatorversion="0.2.1" type="song" version="1.0" >
  <head>
    <automation-pattern>
      <bpm>
        <time value="400" pos="0" />
      </bpm>
      <mastervol>
        <time value="100" pos="0" />
      </mastervol>
      <masterpitch>
        <time value="0" pos="0" />
      </masterpitch>
    </automation-pattern>
  </head>
  <song>
    <trackcontainer width="1256" x="-1" y="64" height="723" type="songeditor" visible="1" >
      <track muted="0" height="32" type="0" >
        <instrumenttrack width="250" x="2" y="63" height="436" name="Default" tab="0" visible="0" >
          <automation-pattern>
            <vol>
              <time value="100" pos="0" />
            </vol>
            <surpos-x>
              <time value="0" pos="0" />
            </surpos-x>
            <surpos-y>
              <time value="0" pos="0" />
            </surpos-y>
            <fxch>
              <time value="0" pos="0" />
            </fxch>
            <basenote>
              <time value="57" pos="0" />
            </basenote>
          </automation-pattern>
          <tripleoscillator userwavefile1="" userwavefile2="" userwavefile0="" >
            <automation-pattern>
              <modalgo1>
                <time value="2" pos="0" />
              </modalgo1>
              <modalgo2>
                <time value="2" pos="0" />
              </modalgo2>
              <vol0>
                <time value="33" pos="0" />
              </vol0>
              <pan0>
                <time value="0" pos="0" />
              </pan0>
              <coarse0>
                <time value="0" pos="0" />
              </coarse0>
              <finel0>
                <time value="0" pos="0" />
              </finel0>
              <finer0>
                <time value="0" pos="0" />
              </finer0>
              <phoffset0>
                <time value="0" pos="0" />
              </phoffset0>
              <stphdetun0>
                <time value="0" pos="0" />
              </stphdetun0>
              <wavetype0>
                <time value="0" pos="0" />
              </wavetype0>
              <vol1>
                <time value="33" pos="0" />
              </vol1>
              <pan1>
                <time value="0" pos="0" />
              </pan1>
              <coarse1>
                <time value="0" pos="0" />
              </coarse1>
              <finel1>
                <time value="0" pos="0" />
              </finel1>
              <finer1>
                <time value="0" pos="0" />
              </finer1>
              <phoffset1>
                <time value="0" pos="0" />
              </phoffset1>
              <stphdetun1>
                <time value="0" pos="0" />
              </stphdetun1>
              <wavetype1>
                <time value="0" pos="0" />
              </wavetype1>
              <vol2>
                <time value="33" pos="0" />
              </vol2>
              <pan2>
                <time value="0" pos="0" />
              </pan2>
              <coarse2>
                <time value="0" pos="0" />
              </coarse2>
              <finel2>
                <time value="0" pos="0" />
              </finel2>
              <finer2>
                <time value="0" pos="0" />
              </finer2>
              <phoffset2>
                <time value="0" pos="0" />
              </phoffset2>
              <stphdetun2>
                <time value="0" pos="0" />
              </stphdetun2>
              <wavetype2>
                <time value="0" pos="0" />
              </wavetype2>
            </automation-pattern>
          </tripleoscillator>
          <eldata fwet="0" >
            <automation-pattern>
              <ftype>
                <time value="0" pos="0" />
              </ftype>
              <fcut>
                <time value="14000" pos="0" />
              </fcut>
              <fres>
                <time value="0.5" pos="0" />
              </fres>
            </automation-pattern>
            <elvol lfosyncmode="0" userwavefile="" >
              <automation-pattern>
                <pdel>
                  <time value="0" pos="0" />
                </pdel>
                <att>
                  <time value="0" pos="0" />
                </att>
                <hold>
                  <time value="0.5" pos="0" />
                </hold>
                <dec>
                  <time value="0.5" pos="0" />
                </dec>
                <sus>
                  <time value="0.5" pos="0" />
                </sus>
                <rel>
                  <time value="0.1" pos="0" />
                </rel>
                <amt>
                  <time value="0" pos="0" />
                </amt>
                <lshp>
                  <time value="0" pos="0" />
                </lshp>
                <lpdel>
                  <time value="0" pos="0" />
                </lpdel>
                <latt>
                  <time value="0" pos="0" />
                </latt>
                <lspd>
                  <time value="0.1" pos="0" />
                </lspd>
                <lamt>
                  <time value="0" pos="0" />
                </lamt>
                <x100>
                  <time value="0" pos="0" />
                </x100>
                <ctlenvamt>
                  <time value="0" pos="0" />
                </ctlenvamt>
              </automation-pattern>
            </elvol>
            <elcut lfosyncmode="0" userwavefile="" >
              <automation-pattern>
                <pdel>
                  <time value="0" pos="0" />
                </pdel>
                <att>
                  <time value="0" pos="0" />
                </att>
                <hold>
                  <time value="0.5" pos="0" />
                </hold>
                <dec>
                  <time value="0.5" pos="0" />
                </dec>
                <sus>
                  <time value="0.5" pos="0" />
                </sus>
                <rel>
                  <time value="0.1" pos="0" />
                </rel>
                <amt>
                  <time value="0" pos="0" />
                </amt>
                <lshp>
                  <time value="0" pos="0" />
                </lshp>
                <lpdel>
                  <time value="0" pos="0" />
                </lpdel>
                <latt>
                  <time value="0" pos="0" />
                </latt>
                <lspd>
                  <time value="0.1" pos="0" />
                </lspd>
                <lamt>
                  <time value="0" pos="0" />
                </lamt>
                <x100>
                  <time value="0" pos="0" />
                </x100>
                <ctlenvamt>
                  <time value="0" pos="0" />
                </ctlenvamt>
              </automation-pattern>
            </elcut>
            <elres lfosyncmode="0" userwavefile="" >
              <automation-pattern>
                <pdel>
                  <time value="0" pos="0" />
                </pdel>
                <att>
                  <time value="0" pos="0" />
                </att>
                <hold>
                  <time value="0.5" pos="0" />
                </hold>
                <dec>
                  <time value="0.5" pos="0" />
                </dec>
                <sus>
                  <time value="0.5" pos="0" />
                </sus>
                <rel>
                  <time value="0.1" pos="0" />
                </rel>
                <amt>
                  <time value="0" pos="0" />
                </amt>
                <lshp>
                  <time value="0" pos="0" />
                </lshp>
                <lpdel>
                  <time value="0" pos="0" />
                </lpdel>
                <latt>
                  <time value="0" pos="0" />
                </latt>
                <lspd>
                  <time value="0.1" pos="0" />
                </lspd>
                <lamt>
                  <time value="0" pos="0" />
                </lamt>
                <x100>
                  <time value="0" pos="0" />
                </x100>
                <ctlenvamt>
                  <time value="0" pos="0" />
                </ctlenvamt>
              </automation-pattern>
            </elres>
          </eldata>
          <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
            <automation-pattern>
              <chord>
                <time value="0" pos="0" />
              </chord>
              <chordrange>
                <time value="1" pos="0" />
              </chordrange>
              <arp>
                <time value="0" pos="0" />
              </arp>
              <arprange>
                <time value="1" pos="0" />
              </arprange>
              <arptime>
                <time value="100" pos="0" />
              </arptime>
              <arpgate>
                <time value="100" pos="0" />
              </arpgate>
              <arpdir>
                <time value="0" pos="0" />
              </arpdir>
              <arpmode>
                <time value="0" pos="0" />
              </arpmode>
            </automation-pattern>
          </arpandchords>
          <midi>
            <automation-pattern>
              <inputchannel>
                <time value="0" pos="0" />
              </inputchannel>
              <outputchannel>
                <time value="1" pos="0" />
              </outputchannel>
              <receive>
                <time value="0" pos="0" />
              </receive>
              <send>
                <time value="0" pos="0" />
              </send>
              <defvelin>
                <time value="0" pos="0" />
              </defvelin>
              <defvelout>
                <time value="0" pos="0" />
              </defvelout>
            </automation-pattern>
          </midi>
        </instrumenttrack>
      </track>
      <track muted="0" height="32" type="2" >
        <sampletrack icon="" name="Sample track" >
          <automation-pattern>
            <vol>
              <time value="100" pos="0" />
            </vol>
          </automation-pattern>
        </sampletrack>
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="kick" >
          <trackcontainer width="504" x="285" y="561" height="198" type="bbeditor" visible="1" >
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="576" y="63" height="436" name="Default" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <tripleoscillator userwavefile1="" userwavefile2="" userwavefile0="" >
                  <automation-pattern>
                    <modalgo1>
                      <time value="2" pos="0" />
                    </modalgo1>
                    <modalgo2>
                      <time value="2" pos="0" />
                    </modalgo2>
                    <vol0>
                      <time value="33" pos="0" />
                    </vol0>
                    <pan0>
                      <time value="0" pos="0" />
                    </pan0>
                    <coarse0>
                      <time value="0" pos="0" />
                    </coarse0>
                    <finel0>
                      <time value="0" pos="0" />
                    </finel0>
                    <finer0>
                      <time value="0" pos="0" />
                    </finer0>
                    <phoffset0>
                      <time value="0" pos="0" />
                    </phoffset0>
                    <stphdetun0>
                      <time value="0" pos="0" />
                    </stphdetun0>
                    <wavetype0>
                      <time value="0" pos="0" />
                    </wavetype0>
                    <vol1>
                      <time value="33" pos="0" />
                    </vol1>
                    <pan1>
                      <time value="0" pos="0" />
                    </pan1>
                    <coarse1>
                      <time value="0" pos="0" />
                    </coarse1>
                    <finel1>
                      <time value="0" pos="0" />
                    </finel1>
                    <finer1>
                      <time value="0" pos="0" />
                    </finer1>
                    <phoffset1>
                      <time value="0" pos="0" />
                    </phoffset1>
                    <stphdetun1>
                      <time value="0" pos="0" />
                    </stphdetun1>
                    <wavetype1>
                      <time value="0" pos="0" />
                    </wavetype1>
                    <vol2>
                      <time value="33" pos="0" />
                    </vol2>
                    <pan2>
                      <time value="0" pos="0" />
                    </pan2>
                    <coarse2>
                      <time value="0" pos="0" />
                    </coarse2>
                    <finel2>
                      <time value="0" pos="0" />
                    </finel2>
                    <finer2>
                      <time value="0" pos="0" />
                    </finer2>
                    <phoffset2>
                      <time value="0" pos="0" />
                    </phoffset2>
                    <stphdetun2>
                      <time value="0" pos="0" />
                    </stphdetun2>
                    <wavetype2>
                      <time value="0" pos="0" />
                    </wavetype2>
                  </automation-pattern>
                </tripleoscillator>
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="Default" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="Default" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="Default" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="Default" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="Default" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="Default" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="Default" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="Default" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="Default" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="Default" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="Default" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="Default" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="Default" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="Default" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="Default" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="760" y="463" height="436" name="kick_hardcore01.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="139" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999079" sframe="0" amp="100" src="drums/kick_hardcore01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="1" name="kick_hardcore01.ogg" pos="0" frozen="0" len="128" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="32" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="64" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="80" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="88" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="96" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="112" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="1" name="kick_hardcore01.ogg" pos="64" frozen="0" len="64" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="32" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="1" name="kick_hardcore01.ogg" pos="128" frozen="0" len="64" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="32" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="48" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="0" name="kick_hardcore01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_hardcore01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_hardcore01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_hardcore01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_hardcore01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_hardcore01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_hardcore01.ogg" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_hardcore01.ogg" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_hardcore01.ogg" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_hardcore01.ogg" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_hardcore01.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_hardcore01.ogg" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="760" y="63" height="436" name="techno_synth01.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.99894" sframe="0" amp="100" src="basses/techno_synth01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="techno_synth01.ogg" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="670" y="463" height="436" name="bassdrum_acoustic02.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999822" sframe="0" amp="100" src="drums/bassdrum_acoustic02.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bassdrum_acoustic02.ogg" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="2" y="463" height="436" name="clap04.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="88" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.998985" sframe="0" amp="100" src="drums/clap04.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="clap04.ogg" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="760" y="63" height="436" name="hihat_closed02.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="22" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.996564" sframe="0" amp="100" src="drums/hihat_closed02.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="hihat_closed02.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_closed02.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_closed02.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="1" name="hihat_closed02.ogg" pos="192" frozen="0" len="64" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="32" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="48" len="4" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="0" name="hihat_closed02.ogg" pos="256" frozen="0" len="64" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="16" len="-64" />
                <note tone="9" pan="0" oct="4" vol="100" pos="48" len="-64" />
              </pattern>
              <pattern steps="16" muted="0" type="0" name="hihat_closed02.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_closed02.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_closed02.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_closed02.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_closed02.ogg" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_closed02.ogg" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_closed02.ogg" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_closed02.ogg" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_closed02.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_closed02.ogg" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="255" y="463" height="436" name="hihat_opened01.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="54" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999262" sframe="0" amp="100" src="drums/hihat_opened01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="320" frozen="0" len="64" >
                <note tone="9" pan="0" oct="4" vol="100" pos="32" len="-64" />
              </pattern>
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="hihat_opened01.ogg" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="255" y="63" height="436" name="church_organ04.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999963" sframe="0" amp="100" src="instruments/church_organ04.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="church_organ04.ogg" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="506" y="414" height="436" name="harpsichord01.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999894" sframe="0" amp="100" src="instruments/harpsichord01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="harpsichord01.ogg" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="2" y="443" height="436" name="piano02.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="40" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999977" sframe="0" amp="100" src="instruments/piano02.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="1" name="piano02.ogg" pos="384" frozen="0" len="512" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="4" vol="100" pos="64" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="128" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="3" pan="0" oct="4" vol="100" pos="192" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="4" vol="100" pos="256" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="6" pan="0" oct="4" vol="100" pos="320" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="4" vol="100" pos="384" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="4" vol="100" pos="448" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="4" vol="100" pos="480" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="1" name="piano02.ogg" pos="448" frozen="0" len="512" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="4" vol="100" pos="64" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="128" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="3" pan="0" oct="4" vol="100" pos="192" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="4" vol="100" pos="256" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="6" pan="0" oct="4" vol="100" pos="320" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="4" vol="100" pos="384" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="7" pan="0" oct="4" vol="100" pos="416" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="448" len="64" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="1" name="piano02.ogg" pos="512" frozen="0" len="256" >
                <note tone="4" pan="0" oct="5" vol="96" pos="0" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="5" vol="100" pos="16" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="16" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="32" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="5" vol="100" pos="48" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="48" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="64" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="5" pan="0" oct="5" vol="100" pos="80" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="80" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="96" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="112" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="112" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="128" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="5" vol="100" pos="144" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="144" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="5" pan="0" oct="5" vol="100" pos="160" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="160" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="176" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="5" vol="100" pos="192" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="192" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="208" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="3" pan="0" oct="5" vol="100" pos="224" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="4" vol="100" pos="224" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="4" vol="100" pos="240" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="1" name="piano02.ogg" pos="576" frozen="0" len="256" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="5" vol="100" pos="0" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="16" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="5" vol="100" pos="16" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="32" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="48" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="5" vol="100" pos="48" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="64" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="3" pan="0" oct="5" vol="100" pos="80" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="80" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="96" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="112" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="112" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="128" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="3" pan="0" oct="5" vol="100" pos="144" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="144" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="160" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="5" vol="100" pos="176" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="176" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="192" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="3" pan="0" oct="5" vol="100" pos="208" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="208" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="2" pan="0" oct="5" vol="100" pos="224" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="4" vol="100" pos="224" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="4" pan="0" oct="4" vol="100" pos="240" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="1" pan="0" oct="5" vol="100" pos="240" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="piano02.ogg" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="506" y="34" height="436" name="bass_hard02.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999825" sframe="0" amp="100" src="basses/bass_hard02.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass_hard02.ogg" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="305" y="463" height="436" name="bass01.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999049" sframe="0" amp="100" src="basses/bass01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="bass01.ogg" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="2" y="34" height="436" name="snare_acoustic01.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.998327" sframe="0" amp="100" src="drums/snare_acoustic01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_acoustic01.ogg" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="305" y="34" height="436" name="snare_muffled01.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999692" sframe="0" amp="100" src="drums/snare_muffled01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="snare_muffled01.ogg" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="508" y="434" height="436" name="tom01.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999692" sframe="0" amp="100" src="drums/tom01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="640" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="704" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="768" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="tom01.ogg" pos="896" frozen="0" len="64" />
            </track>
            <track muted="0" height="32" type="0" >
              <instrumenttrack width="250" x="51" y="434" height="436" name="kick_distorted01.ogg" tab="0" visible="0" >
                <automation-pattern>
                  <vol>
                    <time value="100" pos="0" />
                  </vol>
                  <surpos-x>
                    <time value="0" pos="0" />
                  </surpos-x>
                  <surpos-y>
                    <time value="0" pos="0" />
                  </surpos-y>
                  <fxch>
                    <time value="0" pos="0" />
                  </fxch>
                  <basenote>
                    <time value="57" pos="0" />
                  </basenote>
                </automation-pattern>
                <audiofileprocessor reversed="0" looped="0" eframe="0.999597" sframe="0" amp="100" src="drums/kick_distorted01.ogg" />
                <eldata fwet="0" >
                  <automation-pattern>
                    <ftype>
                      <time value="0" pos="0" />
                    </ftype>
                    <fcut>
                      <time value="14000" pos="0" />
                    </fcut>
                    <fres>
                      <time value="0.5" pos="0" />
                    </fres>
                  </automation-pattern>
                  <elvol lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elvol>
                  <elcut lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elcut>
                  <elres lfosyncmode="0" userwavefile="" >
                    <automation-pattern>
                      <pdel>
                        <time value="0" pos="0" />
                      </pdel>
                      <att>
                        <time value="0" pos="0" />
                      </att>
                      <hold>
                        <time value="0.5" pos="0" />
                      </hold>
                      <dec>
                        <time value="0.5" pos="0" />
                      </dec>
                      <sus>
                        <time value="0.5" pos="0" />
                      </sus>
                      <rel>
                        <time value="0.1" pos="0" />
                      </rel>
                      <amt>
                        <time value="0" pos="0" />
                      </amt>
                      <lshp>
                        <time value="0" pos="0" />
                      </lshp>
                      <lpdel>
                        <time value="0" pos="0" />
                      </lpdel>
                      <latt>
                        <time value="0" pos="0" />
                      </latt>
                      <lspd>
                        <time value="0.1" pos="0" />
                      </lspd>
                      <lamt>
                        <time value="0" pos="0" />
                      </lamt>
                      <x100>
                        <time value="0" pos="0" />
                      </x100>
                      <ctlenvamt>
                        <time value="0" pos="0" />
                      </ctlenvamt>
                    </automation-pattern>
                  </elres>
                </eldata>
                <arpandchords arpdisabled="1" chorddisabled="1" arpsyncmode="0" >
                  <automation-pattern>
                    <chord>
                      <time value="0" pos="0" />
                    </chord>
                    <chordrange>
                      <time value="1" pos="0" />
                    </chordrange>
                    <arp>
                      <time value="0" pos="0" />
                    </arp>
                    <arprange>
                      <time value="1" pos="0" />
                    </arprange>
                    <arptime>
                      <time value="100" pos="0" />
                    </arptime>
                    <arpgate>
                      <time value="100" pos="0" />
                    </arpgate>
                    <arpdir>
                      <time value="0" pos="0" />
                    </arpdir>
                    <arpmode>
                      <time value="0" pos="0" />
                    </arpmode>
                  </automation-pattern>
                </arpandchords>
                <midi>
                  <automation-pattern>
                    <inputchannel>
                      <time value="0" pos="0" />
                    </inputchannel>
                    <outputchannel>
                      <time value="1" pos="0" />
                    </outputchannel>
                    <receive>
                      <time value="0" pos="0" />
                    </receive>
                    <send>
                      <time value="0" pos="0" />
                    </send>
                    <defvelin>
                      <time value="0" pos="0" />
                    </defvelin>
                    <defvelout>
                      <time value="0" pos="0" />
                    </defvelout>
                  </automation-pattern>
                </midi>
              </instrumenttrack>
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="0" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="64" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="128" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="192" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="256" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="320" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="384" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="448" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="512" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="576" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="1" name="kick_distorted01.ogg" pos="640" frozen="0" len="128" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="32" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="64" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="80" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="88" len="8" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="96" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="112" len="12" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="1" name="kick_distorted01.ogg" pos="704" frozen="0" len="64" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="32" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="1" name="kick_distorted01.ogg" pos="768" frozen="0" len="64" >
                <note tone="9" pan="0" oct="4" vol="100" pos="0" len="32" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="32" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
                <note tone="9" pan="0" oct="4" vol="100" pos="48" len="16" >
                  <automation-pattern>
                    <detuning>
                      <time value="0" pos="0" />
                    </detuning>
                  </automation-pattern>
                </note>
              </pattern>
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="832" frozen="0" len="64" />
              <pattern steps="16" muted="0" type="0" name="kick_distorted01.ogg" pos="896" frozen="0" len="64" />
            </track>
          </trackcontainer>
        </bbtrack>
        <bbtco muted="0" name="Beat/Baseline 0" color="4282417407" pos="256" len="64" />
        <bbtco muted="0" name="Beat/Baseline 0" color="4282417407" pos="768" len="128" />
        <bbtco muted="0" name="Beat/Baseline 0" color="4282417407" pos="1280" len="128" />
        <bbtco muted="0" name="kick" color="4282417407" pos="1792" len="128" />
        <bbtco muted="0" name="kick" color="4282417407" pos="2368" len="128" />
        <bbtco muted="0" name="kick" color="4282417407" pos="2944" len="128" />
        <bbtco muted="0" name="kick" color="4282417407" pos="3968" len="128" />
        <bbtco muted="0" name="kick" color="4282417407" pos="4288" len="64" />
        <bbtco muted="0" name="kick" color="4282417407" pos="4544" len="64" />
        <bbtco muted="0" name="kick" color="4282417407" pos="4800" len="320" />
        <bbtco muted="0" name="kick" color="4282417407" pos="384" len="64" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="kick" />
        <bbtco muted="0" name="Beat/Baseline 1" color="4282417407" pos="0" len="64" />
        <bbtco muted="0" name="Beat/Baseline 1" color="4282417407" pos="64" len="64" />
        <bbtco muted="0" name="Beat/Baseline 1" color="4282417407" pos="128" len="64" />
        <bbtco muted="0" name="Beat/Baseline 1" color="4282417407" pos="512" len="64" />
        <bbtco muted="0" name="Beat/Baseline 1" color="4282417407" pos="576" len="64" />
        <bbtco muted="0" name="Beat/Baseline 1" color="4282417407" pos="640" len="64" />
        <bbtco muted="0" name="Beat/Baseline 1" color="4282417407" pos="960" len="64" />
        <bbtco muted="0" name="Beat/Baseline 1" color="4282417407" pos="1024" len="64" />
        <bbtco muted="0" name="Beat/Baseline 1" color="4282417407" pos="1088" len="64" />
        <bbtco muted="0" name="Beat/Baseline 1" color="4282417407" pos="1152" len="64" />
        <bbtco muted="0" name="Beat/Baseline 1" color="4282417407" pos="1472" len="64" />
        <bbtco muted="0" name="kick" color="4282417407" pos="1536" len="64" />
        <bbtco muted="0" name="kick" color="4282417407" pos="1600" len="64" />
        <bbtco muted="0" name="kick" color="4282417407" pos="1664" len="64" />
        <bbtco muted="0" name="kick" color="4282417407" pos="2496" len="320" />
        <bbtco muted="0" name="kick" color="4282417407" pos="1984" len="64" />
        <bbtco muted="0" name="kick" color="4282417407" pos="3456" len="64" />
        <bbtco muted="0" name="kick" color="4282417407" pos="3840" len="64" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="kick" />
        <bbtco muted="0" name="Beat/Baseline 2" color="4282417407" pos="192" len="64" />
        <bbtco muted="0" name="Beat/Baseline 2" color="4282417407" pos="704" len="64" />
        <bbtco muted="0" name="Beat/Baseline 2" color="4282417407" pos="896" len="64" />
        <bbtco muted="0" name="Beat/Baseline 2" color="4282417407" pos="1216" len="64" />
        <bbtco muted="0" name="Beat/Baseline 2" color="4282417407" pos="1408" len="64" />
        <bbtco muted="0" name="kick" color="4282417407" pos="1920" len="64" />
        <bbtco muted="0" name="kick" color="4282417407" pos="1728" len="64" />
        <bbtco muted="0" name="kick" color="4282417407" pos="2048" len="320" />
        <bbtco muted="0" name="kick" color="4282417407" pos="2816" len="128" />
        <bbtco muted="0" name="kick" color="4282417407" pos="3584" len="64" />
        <bbtco muted="0" name="kick" color="4282417407" pos="3712" len="64" />
        <bbtco muted="0" name="kick" color="4282417407" pos="4096" len="192" />
        <bbtco muted="0" name="kick" color="4282417407" pos="4352" len="192" />
        <bbtco muted="0" name="kick" color="4282417407" pos="4608" len="192" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Beat/Baseline 3" />
        <bbtco muted="0" name="Beat/Baseline 3" color="4282417407" pos="3072" len="1536" />
        <bbtco muted="0" name="Beat/Baseline 3" color="4282417407" pos="1536" len="448" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="hi close" />
        <bbtco muted="0" name="Beat/Baseline 4" color="4282417407" pos="512" len="1024" />
        <bbtco muted="0" name="hi close" color="4282417407" pos="1856" len="1216" />
        <bbtco muted="0" name="hi close" color="4282417407" pos="3968" len="1152" />
        <bbtco muted="0" name="hi close" color="4282417407" pos="320" len="192" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="hi open" />
        <bbtco muted="0" name="Beat/Baseline 5" color="4282417407" pos="512" len="1024" />
        <bbtco muted="0" name="hi open" color="4282417407" pos="1984" len="1088" />
        <bbtco muted="0" name="hi open" color="4282417407" pos="4096" len="1024" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Beat/Baseline 6" />
        <bbtco muted="0" name="Beat/Baseline 6" color="4282417407" pos="1024" len="512" />
        <bbtco muted="0" name="Beat/Baseline 6" color="4282417407" pos="3072" len="512" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Beat/Baseline 7" />
        <bbtco muted="0" name="Beat/Baseline 7" color="4282417407" pos="1536" len="512" />
        <bbtco muted="0" name="Beat/Baseline 7" color="4282417407" pos="3584" len="512" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Beat/Baseline 9" />
        <bbtco muted="0" name="Beat/Baseline 9" color="4282417407" pos="2048" len="256" />
        <bbtco muted="0" name="Beat/Baseline 9" color="4282417407" pos="2560" len="256" />
        <bbtco muted="0" name="Beat/Baseline 9" color="4282417407" pos="4096" len="256" />
        <bbtco muted="0" name="Beat/Baseline 9" color="4282417407" pos="4608" len="256" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Beat/Baseline 9" />
        <bbtco muted="0" name="Beat/Baseline 9" color="4282417407" pos="2304" len="256" />
        <bbtco muted="0" name="Beat/Baseline 9" color="4282417407" pos="2816" len="256" />
        <bbtco muted="0" name="Beat/Baseline 9" color="4282417407" pos="4352" len="256" />
        <bbtco muted="0" name="Beat/Baseline 9" color="4282417407" pos="4864" len="256" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Beat/Baseline 10" />
        <bbtco muted="0" name="Beat/Baseline 10" color="4282417407" pos="3712" len="128" />
        <bbtco muted="0" name="Beat/Baseline 10" color="4282417407" pos="4480" len="128" />
        <bbtco muted="0" name="Beat/Baseline 10" color="4282417407" pos="4864" len="128" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Beat/Baseline 11" />
        <bbtco muted="0" name="Beat/Baseline 11" color="4282417407" pos="3072" len="384" />
        <bbtco muted="0" name="Beat/Baseline 11" color="4282417407" pos="3584" len="128" />
        <bbtco muted="0" name="Beat/Baseline 11" color="4282417407" pos="3840" len="256" />
        <bbtco muted="0" name="Beat/Baseline 11" color="4282417407" pos="4224" len="256" />
        <bbtco muted="0" name="Beat/Baseline 11" color="4282417407" pos="4608" len="256" />
        <bbtco muted="0" name="Beat/Baseline 11" color="4282417407" pos="5056" len="64" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Beat/Baseline 12" />
        <bbtco muted="0" name="Beat/Baseline 12" color="4282417407" pos="3456" len="128" />
        <bbtco muted="0" name="Beat/Baseline 12" color="4282417407" pos="4096" len="128" />
        <bbtco muted="0" name="Beat/Baseline 12" color="4282417407" pos="4992" len="64" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Beat/Baseline 13" />
        <bbtco muted="0" name="Beat/Baseline 13" color="4282417407" pos="4096" len="256" />
        <bbtco muted="0" name="Beat/Baseline 13" color="4282417407" pos="4608" len="256" />
      </track>
      <track muted="0" height="32" type="1" >
        <bbtrack icon="" name="Beat/Baseline 14" />
      </track>
    </trackcontainer>
    <pianoroll width="640" x="208" y="54" height="475" visible="0" />
    <automation-editor width="640" x="2" y="148" height="480" visible="0" />
    <projectnotes width="300" x="2" y="384" height="200" visible="0" ><![CDATA[<html><head><meta name="qrichtext" content="1" /></head><body style="font-size:9pt;font-family:Sans Serif">
<p>Put down your project notes here.</p>
</body></html>
]]></projectnotes>
    <timeline lp1pos="5120" lp0pos="0" lpstate="1" />
  </song>
</multimediaproject>
